>> MIB - Management Information Base
>> Table: ipSifAliasAddressTable - (.1.3.6.1.4.1.272.4.5.28.1)
Description: Contents a Stateful inspection Firewall description for a alias Name
ipSifAliasAddressTable
OID | Name | Type | Access
.1 | Index | INTEGER | R
.2 | Alias | DisplayString | RW
.3 | Address | IpAddress | RW
.4 | Mask | IpAddress | RW
.5 | Interface | INTEGER | RW
.6 | Mode | ENUM | D
.7 | Range | INTEGER | RW
.8 | Group | INTEGER | RW
Index
The Index for the address alias
Alias
Alias Name for the Address Entry Length: 0 to 255
Address
The ip-address for the Alias
Mask
The ip Mask for the Alias
Interface
The interface index for the alias
Mode
Address or Interface Mode Enumerations: interface (1) address (2) range (3) delete (4)
Range
The ip Range for the Alias Range: 0 to 65535
Group
For values greater than zero this entry determines the IP address group this entry belongs to, see also ipSifAliasAddressGroupId

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH