>> MIB - Management Information Base
>> Table: mlpppStatTable - (.1.3.6.1.4.1.272.4.3.16.1)
Description: The mlpppStatTable contains statistical multilink specific information. Only the system can add or delete entries to this table. Creating entries: Entries are created by the system each time a new multilink PPP interface is negotiated. Deleting entries: Entries are removed by the system when the multilink feature is disabled.
mlpppStatTable
OID | Name | Type | Access
.1 | IfIndex | INTEGER | R
.2 | NextTxSeqno | INTEGER | R
.3 | LastRxSeqno | INTEGER | R
.4 | MaxFragCount | INTEGER | R
.5 | MaxFragLifeTime | INTEGER | R
.6 | FragsRcvd | Counter | R
.7 | FragsQueued | Counter | R
.8 | FragsDropped | Counter | R
.9 | PktsReassembled | Counter | R
.10 | BeginOfQueue | INTEGER | R
.11 | EndOfQueue | INTEGER | R
.12 | BFragsQueued | INTEGER | R
.13 | EFragsQueued | INTEGER | R
.14 | MFragsQueued | INTEGER | R
.15 | CFragsQueued | INTEGER | R
.16 | AgeDrops | Counter | R
.17 | OutOfSyncDrops | Counter | R
.18 | OverFlowDrops | Counter | R
.19 | DuplicateDrops | Counter | R
.20 | ForwardDeviation | INTEGER | R
.21 | BackwardDeviation | INTEGER | R
.22 | NextReasSeqNo | INTEGER | R
.23 | OutOfOrderWaits | INTEGER | R
.24 | MaxReasBurst | INTEGER | R
.25 | CleanupDrops | Counter | R
IfIndex
Correlating PPP interface index.
NextTxSeqno
description not available Range: 0 to 16777215
LastRxSeqno
description not available Range: 0 to 16777215
MaxFragCount
Maximum size (number of Fragments) of MLPPP reassembling area. Range: 0 to 10000
MaxFragLifeTime
Maximum lifetime of fragments stored in MLPPP reassembling area. Range: 0 to 10
FragsRcvd
Total number of MLPPP fragments received since interface is in operational 'up' status.
FragsQueued
Current number of MLPPP fragments stored in MLPPP reassembling area.
FragsDropped
Total number of MLPPP fragments dropped since interface is in operational 'up' status.
PktsReassembled
Total number pakets reassembled since interface is in operational 'up' status.
BeginOfQueue
Sequence Number of first fragment stored in MLPPP reassembling area. Range: 0 to 16777215
EndOfQueue
Sequence Number of last fragment stored in MLPPP reassembling area. Range: 0 to 16777215
BFragsQueued
Current number (begin-)fragments stored in MLPPP reassembling area. Range: 0 to 10000
EFragsQueued
Current number (end-)fragments stored in MLPPP reassembling area. Range: 0 to 10000
MFragsQueued
Current number (middle-)fragments stored in MLPPP reassembling area. Range: 0 to 10000
CFragsQueued
Current number (complete-)fragments stored in MLPPP reassembling area. Range: 0 to 10000
AgeDrops
Total number fragments dropped due to exceeded lifetime, see also mlpppMaxFragLifeTime.
OutOfSyncDrops
Total number fragments dropped due to a 'out of sync' condition.
OverFlowDrops
Total number fragments dropped due to a MLPPP reassembling area 'overflow' condition, see also mlpppMaxFragCount.
DuplicateDrops
Total number duplicate fragments dropped.
ForwardDeviation
Maximum deviation of current received sequence number compared with the end of the reassembling queue in forward direction. Range: 0 to 10000
BackwardDeviation
Maximum deviation of current received sequence number compared with the begin of the reassembling queue in backward direction. Range: 0 to 10000
NextReasSeqNo
Awaited first sequence number of next the fragment chain or packet ready to be distributed to the upper layer. Range: 0 to 16777215
OutOfOrderWaits
Number of cycles already reassembled packets are retained due to the expected mlpppNextReasSeqNo value.
MaxReasBurst
Maximum number of reassembled packets sended to the upper layer within one cycle. Range: 0 to 16777215
CleanupDrops
Number of fragments dropped cause they were still in in the queue when interface went down.

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH