>> MIB - Management Information Base
>> Table: ipsecPeerTable - (.1.3.6.1.4.1.272.4.26.5.1)
Description: This object contains the description of an IPSec peer.
ipsecPeerTable
OID | Name | Type | Access
.1 | Index | INTEGER | R
.3 | Description | DisplayString | RW
.5 | PeerIds | DisplayString | RW
.8 | LocalAddress | IpAddress | RW
.11 | TrafficList | INTEGER | RW
.14 | DynamicAddress | DisplayString | RW
.15 | VirtualInterface | ENUM | RW
.16 | StartMode | ENUM | RW
.21 | PreSharedKey | DisplayString | RW
.45 | IsdnCB | ENUM | RW
.47 | Priority | INTEGER | RW
.48 | IkeProfile | INTEGER | RW
.49 | IpsecProfile | INTEGER | RW
.50 | AdminStatus | ENUM | D
.63 | PreSharedKeyData | OCTET STRING | N
.66 | IsdnCBMode | ENUM | RW
.67 | IsdnCBDChanMode | ENUM | RW
.73 | Type | ENUM | RW
.78 | DynAddrPoolId | INTEGER | RW
.79 | DynAddrLocalIp | IpAddress | RW
.80 | XauthProfile | Unsigned32 | RW
.81 | DynAddrRole | ENUM | RW
.82 | IkeVersion | ENUM | RW
.83 | LocalId | DisplayString | RW
.84 | AuthMethod | ENUM | RW
.85 | Cert | INTEGER | RW
.86 | CaCerts | DisplayString | RW
.87 | DynAddrMode | ENUM | RW
.88 | Mobike | ENUM | RW
.89 | IpVersion | ENUM | RW
.90 | PublicIfIndex | INTEGER | RW
.91 | PublicIfIndexMode | ENUM | RW
Index
A unique index identifying this entry.
Description
An optional description for this peer. Length: 0 to 255
PeerIds
The IDs of the peer which are accepted for authentication. Syntax: - X500 distinguished name: <obj-name=obj-value, obj-ID=obj-value, ...> - IPV4-Address: |123.456.789.012| with or without '|' - IPV4 Address Range (only IKEv1): |123.456.789.012-123.456.789.013| with or without '|' - IPV4 Address Subnet (only IKEv1): |123.456.789.012/255.255.255.0| with or without '|' or: |123.456.789.012/24| with or without '|' - Key-ID: arbitrary string: {anything} - Fully Qualified User Name (FQUN) (for IKEv1) or Fully-qualified RFC 822 email address string (for IKEv2): (anything) or user@domain with mandatory '@' - Fully Qualified Domain Name (FQDN): [anything] or any name without '@' not matching any other syntax Length: 0 to 255
LocalAddress
The local address used for IPSec encrypted packets.
TrafficList
This object specifies the first entry of possibly a chain of traffic entries from the ipsecTrafficTable which should be protected with IPSec using this peer.
DynamicAddress
The IP-address of the peer. This object may contain either an IP address or a domain name. Length: 0 to 255
VirtualInterface
This object specifies if a virtual interface should be created for this peer. If set to enabled, all traffic routed towards this peer will be protected. The traffic list for this peer is ignored then. The index of the interface associated with this peer is calculated as follows: ifIndex = ipsecPeerIndex + 100000. Enumerations: disabled (1) enabled (2)
StartMode
This object specifies the events which make the IPSec peer go up. Possible values: on-demand(1), -- packet triggered start, -- fall back to dormant if unused always-up(2) -- always set up and keep up. Enumerations: on-demand (1) always-up (2)
PreSharedKey
The pre-shared-key used with this peer, if pre-shared-keys are used for authentication. This field serves only as an input field and its contents are replaced with a single asterisk immediately after it is set. Length: 0 to 255
IsdnCB
Switch for turning ISDN call back feature on and off specifically for peer. Default value is disabled. Enumerations: enabled (1) disabled (2) passive (3) active (4)
Priority
Defines the matching priority.
IkeProfile
When ipsecPeerIkeVersion is set to ikev1 this is an index from the ikeProfileTable containing a special phase 1 profile to use for this peer. When ipsecPeerIkeVersion is set to ikev2 this is an index from the ikev2ProfileTable containing a special IKE_SA profile to use for this peer.
IpsecProfile
The index from the ipsecProfileTable containing a special phase 2 profile to use for this peer.
AdminStatus
Peer administrative state. Enumerations: up (1) down (2) dialup (4) callback (5) delete (15)
PreSharedKeyData
Field used for storing the pre-shared-key permanently.
IsdnCBMode
Define callback mode. The following modes are defined: compat(1) -- compatibility to old callback auto(2) -- automatically detect best method auto-d(3) -- automatically detect best D channel method d(4) -- use D channel only db(5) -- try D channel first, fall back to B b(6) -- use B channel only Default value for that variable is compat(1). Enumerations: compat (1) auto (2) auto-d (3) d (4) db (5) b (6)
IsdnCBDChanMode
Define callback D channel mode. The following modes are defined: llc(1) -- code token into LLC information element only subaddr(2) -- code token into SUBADDR information element only llc-and-subaddr(3) -- redundantly use LLC and SUBADDR information elements llc-subaddr(4) -- try LLC first, then SUBADDR subaddr-llc(5) -- try SUBADDR first, then LLC Default value for that variable is LLC(1). Enumerations: llc (1) subaddr (2) llc-and-subaddr (3) llc-subaddr (4) subaddr-llc (5)
Type
The type of the peer. Dynamic peer entries are duplicated whenever an incoming IKE request matches the ID and/or address information of the remote side. Note: - For traffic list peers the duplication also includes the traffic list entries configured for this peer entry. - For virtual interface peers, host routes will be added for the peer address automatically. Possible values: fixed(1), -- only one peer allowed for this entry dynamic_client(2) -- duplicated for each incoming client. Enumerations: fixed (1) dynamic-client (2)
DynAddrPoolId
Identifier of Dynamic Address Pool if IP address is assigned via IKE Configuration Method. A value of -1 means that no Pool is assigned. Range: -1 to 65535
DynAddrLocalIp
The local IP address used in the IKE communication when remote IP address is taken from IP address pool.
XauthProfile
The index from the xauthProfileTable containing a special XAUTH profile to use for this peer. A value of 0 means that no XAUTH profile is assigned. Range: 0 to -1
DynAddrRole
Determines if IKE Config Mode is used and which role is performed: none(1), -- no IP address assignemt via IKE Config Mode client(2) -- get IP address via IKE Config Mode from remote server(3) -- assign IP address via IKE Config Mode to remote In server role ipsecPeerDynAddrPoolId defines IP address pool to use for address assignment to clients. If an invalid pool ID is configured, peer is treated as if role was 'none'. Default is 'none', that means IKE Config Mode is not used at all. Enumerations: none (1) client (2) server (3)
IkeVersion
Indicates the major version of IKE protocol to use. If set to ikev1 the value of ipsecPeerIkeProfile is used as index into ikeProfileTable. If set to ikev2 the value of ipsecPeerIkeProfile is used as index into ikev2ProfileTable. Enumerations: ikev1 (1) ikev2 (2)
LocalId
The local ID used for authentication with this profile. Syntax: - X500 distinguished name: <obj-name=obj-value, obj-ID=obj-value, ...> - IPV4-Address: |123.456.789.012| with or without '|' - Key-ID: arbitrary string: {anything} - Fully-qualified RFC 822 email address string: (anything) or user@domain with mandatory '@' - Fully Qualified Domain Name (FQDN): [anything] or any name without '@' not matching any other syntax (only for IKEv2). Length: 0 to 255
AuthMethod
This object specifies the authentication method used by default. If the ipsecPeerAuthMethod field of an ipsecPeerEntry and the ikePropAuthMethod field of the ikeProposalTableEntry used are set to 'default', this value is assumed. Possible values: pre-sh-key(1), -- Authentication using pre shared keys dss-sig(2), -- Authentication using DSS signatures rsa-sig(3) -- Authentication using RSA signatures (only for IKEv2). Enumerations: pre-sh-key (1) dss-sig (2) rsa-sig (3)
Cert
The index of the certificate used for authentication in the certTable. Ignored for AuthMethod == pre_shared_key. (only for IKEv2). Range: 0 to 32767
CaCerts
Receives a comma separated list with indices (0..32767) of special certificate authority certificates accepted for this profile. (only for IKEv2). Length: 0 to 255
DynAddrMode
When IP address assignment via IKE Config Mode is configured (ipsecPeerDynAddrRole != none) this object specifies the used mode: pull(1), -- the client will request IP address and the gateway will answer the request push(2) -- the gateway will set IP address to the client and the client will accept or deny it The ipsecPeerDynAddrMode value has to be the same for both sides of the tunnel. With default value 'pull' the peer (ipsecPeerDynAddrRole == client) will request IP address and the gateway (ipsecPeerDynAddrRole == server) will answer the request. The 'push' mode is needed for partner devices that require this mode. This object matters only when ipsecPeerDynAddrRole != none. Enumerations: pull (1) push (2)
Mobike
This object indicates whether the peer supports MOBIKE or not. Only when both sides of a VPN connection support MOBIKE an IP address change is possible. Possible values: enabled(1), -- Peer supports MOBIKE and signals MOBIKE support by including a MOBIKE_SUPPORTED notification in the IKE_AUTH message. disabled(2) -- Peer does not support MOBIKE. (only for IKEv2). Enumerations: enabled (1) disabled (2)
IpVersion
Determines whether the peer should be connected via IPv4 or via IPv6.
PublicIfIndex
The index value which uniquely identifies the physical interface that should be used for all ipsec traffic as initiator. When multiple eqivalent routes to the given peer are available this is used as additional parameter for routing decisions. If set to -1 then normal routing is used. As responder the interface from the first received packet is used and therefore this index value is ignored.
PublicIfIndexMode
This object defines the mode used in conjunction with ipsecPeerPublicIfIndex. force(1), -- the given interface is used, even if a route with lower metric is available. preferred(2) -- the given interface is used, if no route with lower metric is available. This object matters only when ipsecPeerPublicIfIndex > 0. Enumerations: force (1) preferred (2)

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH