>> MIB - Management Information Base
>> Table: potsIfDataLinkTimerTable - (.1.3.6.1.4.1.272.4.14.1.4.1)
Description: The potsIfDataLinkTimerTable the contains timer values (in ms) controlling on-hook and off-hook data transmission service according to ETSI EN 300 659. The reception of data is controlled with timers according to the minimum and maximum values given in the ETSI standard.
potsIfDataLinkTimerTable
OID | Name | Type | Access
.1 | Index | DataLinkTimerTabIndex | RW
.2 | 0 | INTEGER | RW
.3 | 1 | INTEGER | RW
.4 | 2 | INTEGER | RW
.5 | 3 | INTEGER | RW
.6 | 4 | INTEGER | RW
.7 | 5 | INTEGER | RW
.8 | 6 | INTEGER | RW
.9 | 7 | INTEGER | RW
.10 | 8 | INTEGER | RW
.11 | 9 | INTEGER | RW
.12 | 10 | INTEGER | RW
.13 | 11 | INTEGER | RW
.14 | 12 | INTEGER | RW
.15 | 13 | INTEGER | RW
.16 | 14 | INTEGER | RW
.17 | RpAs | INTEGER | RW
.18 | DtAsOnH | INTEGER | RW
.19 | DtAsOffH | INTEGER | RW
Index
Index of the set of timers which is following up.
0
Timer T0 according to ETSI EN 300 659. Range: 100 to 550
1
Timer T1 according to ETSI EN 300 659. Range: 45 to 500
2
Timer T2 according to ETSI EN 300 659. Range: 200 to 500
3
Timer T3 according to ETSI EN 300 659. Range: 500 to 800
4
Timer T4 according to ETSI EN 300 659. Range: 45 to 500
5
Timer T5 according to ETSI EN 300 659. Range: 500 to 2000
6
Timer T6 according to ETSI EN 300 659. Range: 200 to 3000
7
Timer T7 according to ETSI EN 300 659. Range: 250 to 700
8
Timer T8 according to ETSI EN 300 659. Range: 200 to 500
9
Timer T9 according to ETSI EN 300 659. Range: 0 to 150
10
Timer T10 according to ETSI EN 300 659. Range: 0 to 150
11
Timer T11 according to ETSI EN 300 659. Range: 40 to 55
12
Timer T12 according to ETSI EN 300 659. Range: 55 to 200
13
Timer T13 according to ETSI EN 300 659. Range: 40 to 120
14
Timer T14 according to ETSI EN 300 659. Range: 155 to 165
RpAs
Timer RP-AS according to ETSI EN 300 659. Range: 200 to 300
DtAsOnH
Timer DT-AS on-hook according to ETSI EN 300 659. Range: 90 to 110
DtAsOffH
Timer DT-AS off-hook according to ETSI EN 300 659. Range: 75 to 85

MIB Reference to Software Version 10.1.21 generated on 2016/12/23. Provided by webmaster@bintec-elmeg.com Copyright ©2016 by bintec elmeg GmbH