>> MIB - Management Information Base
>> Table: wlanWMMTable - (.1.3.6.1.4.1.272.4.46.22.1)
Description: Describes a WLAN WMM Access category settings
wlanWMMTable
OID | Name | Type | Access
.1 | AccCat | ENUM | R
.2 | wlanIf | INTEGER | R
.3 | aCWmin | INTEGER | RW
.4 | aCWmax | INTEGER | RW
.5 | Aifsn | INTEGER | RW
.6 | TxopLimitb | INTEGER | RW
.7 | TxopLimitg | INTEGER | RW
.8 | AckPolicy | ENUM | RW
.9 | ACM | ENUM | RW
.10 | Type | ENUM | R
.11 | TxopLimit | INTEGER | RW
AccCat
Access category type, each category is mandatory for a wlanIf. An access category (AC) is a label for the common set of enhanced distributed channel access (EDCA) parameters that are used by a quality of service (QoS) station (QSTA) to contend for the channel in order to transmit medium access control (MAC) service data units (MSDUs) with certain priorities. (More info in '802.11E / 3.123 access category (AC)'). besteffort(1): standard/default priority background(2): low priority video(3): medium priority (higher than 'besteffort') voice(4): high priority Enumerations: besteffort (1) background (2) video (3) voice (4)
wlanIf
Radio index the AC belongs to.
aCWmin
Minimum size of contention window. for AC_BK and AC_BE wlanWMMaCWmin = wlanIfCWmin, for AC_VI wlanWMMaCWmin = (wlanIfCWmin-1)/2, for AC_VO wlanWMMaCWmin = (wlanIfCWmin-3)/4.
aCWmax
Maximum size of contention window. for AC_BK wlanWMMaCWmax = wlanIfCWmax, for AC_BE wlanWMMaCWmax = 4*wlanIfCWmin + 3, for AC_VI wlanWMMaCWmax = wlanIfCWmin, for AC_VO wlanWMMaCWmax = (wlanIfCWmin-1)/2.
Aifsn
Arbitration Inter-Frame Space Number (AIFSN) for this Access category. Range: 0 to 99
TxopLimitb
802.11b mode Transmit Opportunity Limit. Range: 0 to 9999
TxopLimitg
802.11g mode Transmit Opportunity Limit. Range: 0 to 9999
AckPolicy
Ack policy for this Access category (default value is 'ack(1)'). Enumerations: ack (1) noAck (2)
ACM
ACM (admission control) policy for this Access category i (default value is 'disabled(2)'). Enumerations: enabled (1) disabled (2)
Type
Type to which this wlanWMMEntry corresponds. Type access_point means the own parameters for WMM are changed. The entries with type station will be provided to the connected stations via WMM-IE (default value is 'access_point(1)'). Enumerations: access-point (1) station (2)
TxopLimit
802.11 mode Transmit Opportunity Limit. The TxopLimit value is given in units of 32 microseconds.

MIB Reference to Software Version 10.1.21 generated on 2016/12/23. Provided by webmaster@bintec-elmeg.com Copyright ©2016 by bintec elmeg GmbH