>> MIB - Management Information Base
>> Table: wlcDynamicBlacklistProfileTable - (.1.3.6.1.4.1.272.4.61.1.33.1)
Description: The wlcDynamicBlacklistProfile contains information about stations that are blacklisted as a countermeasure to inappropriate behaviour.
wlcDynamicBlacklistProfileTable
OID | Name | Type | Access
.1 | STAMac | MacAddress | R
.2 | VSSProfIndex | INTEGER | R
.3 | FirstSeen | Date | R
.4 | LastSeen | Date | R
.5 | Reason | ENUM | R
.6 | LastRSSI | INTEGER | R
.7 | WTPIndex | INTEGER | R
.8 | RowStatus | ENUM | D
STAMac
The MAC address of the station that is blacklisted. Length: 6 to 6
VSSProfIndex
The SSID on a specific WTP (wlcVSSIndex) a station belongs to.
FirstSeen
The 1st time a blacklisted station drew attention. Range: 0 to -1
LastSeen
The last time a blacklisted station drew attention. Range: 0 to -1
Reason
The reason why a station is blacklisted. Enumerations: badauth (1) invalidFrame (2)
LastRSSI
RSSI of station it annoyed last time.
WTPIndex
The WTP the station was blacklisted at.
RowStatus
The row status of the blacklist entry. Although the conceptual row is not creatable by the user, one is able to set the row to notInService. Enumerations: active (1) notInService (2) notReady (3) createAndGo (4) createAndWait (5) destroy (6)

MIB Reference to Software Version 10.1.21 generated on 2016/12/23. Provided by webmaster@bintec-elmeg.com Copyright ©2016 by bintec elmeg GmbH