>> MIB - Management Information Base
>> Table: vmsAccountTable - (.1.3.6.1.4.1.272.4.34.1.3.1)
Description: This table lists the Voice Account configured for VMS call redirect.
vmsAccountTable
OID | Name | Type | Access
.1 | Index | AccountIndex | RW
.2 | Type | ENUM | RW
.3 | Reference | INTEGER | RW
.4 | Language | ENUM | RW
.5 | Notify | ENUM | RW
.6 | MailTo | DisplayString | RW
.7 | MaxRecordingLength | INTEGER | RW
.8 | CalendarIndex | INTEGER | RW
.9 | AdminStatus | ENUM | D
.10 | OperStatus | ENUM | R
.11 | NewMessages | INTEGER | R
.12 | OldMessages | INTEGER | R
.13 | SavedMessages | INTEGER | R
.14 | MaxMessages | INTEGER | RW
Index
A unique value for each Account. Range: 1 to 65535
Type
Type of account: group or extension. Enumerations: extension (1) group (2)
Reference
This value contains a reference for the voice mail account, it depends on vmsAccountType: - vmsAccountType extension: reference to mpsExtensionTable - vmsAccountType group : reference to mpsGroupTable .
Language
The account-specific language setting for the voice mail server. use-default(99): use language setting from vmsGlobalLanguage. Enumerations: german (1) dutch (2) english (3) italian (5) spanish (7) french (10) portuguese (11) turkish (26) use-default (99)
Notify
Specifies the (admin) mail notification mode: no(1) : no mail is sent mail(2) : send a mail without attachment mail-attachment(3): send a mail with the new message attached use-user-config(4): use settings from vmsAccountUserNotify Enumerations: no (1) mail (2) mail-attachment (3) use-user-config (4)
MailTo
Specifies the notification recipient. If not defined use mail address from mpsUserTable. Length: 0 to 255
MaxRecordingLength
Maximum recording length (in seconds) of the messages for this account. Range: 5 to 300
CalendarIndex
The announcement business or outside business can be switched automatically by a calendar. This is the reference to mpsCalendarTable if active.
AdminStatus
Enable, disable or delete VMS account. Enumerations: enable (1) delete (2) disable (3)
OperStatus
Operational status of the account. Enumerations: up (1) down (2) licMissing (3)
NewMessages
This value contains the number of new messages for this account. Range: 0 to 1000
OldMessages
This value contains the number of old messages for this account. Range: 0 to 1000
SavedMessages
This value contains the number of saved messages for this account. Range: 0 to 1000
MaxMessages
This value contains the maximum number of allowed messages for this account. If this amount is reached, no more recordings are possible. Range: 0 to 1000

MIB Reference to Software Version 10.1.21 generated on 2016/12/23. Provided by webmaster@bintec-elmeg.com Copyright ©2016 by bintec elmeg GmbH