>> MIB - Management Information Base
>> Table: lispMapSrvTable - (.1.3.6.1.4.1.272.4.23.9.4.1)
Description: List of Map-Servers (see section 4.2 of RFC-6833) to inform about configured local LISP-sites.
lispMapSrvTable
OID | Name | Type | Access
.1 | Addr | IpAddress | RW
.2 | AdminStatus | ENUM | D
.3 | Period | Unsigned32 | RW
.4 | NextReg | TimeTicks | R
.5 | KeyId | ENUM | RW
.6 | KeyVal | OCTET STRING | RW
.7 | KeyLen | Unsigned32 | R
.8 | AuthMode | ENUM | RW
.9 | AuthLen | Unsigned32 | R
Addr
RLOC of this Map-Server.
AdminStatus
Administrative status of Map-Server. Set to delete for killing entry. Enumerations: active (1) inactive (2) delete (3)
Period
Period in seconds for Map-Register-frames sent to this Map-Server.
NextReg
Count-down for next Map-Register-send-attempt to this Map-Server. Relevant only if this entry is active and if there is at least one active lispLocSite-entry with related active lispInst-entry.
KeyId
Method and implied key-format used for Map-Register-authentication. Authentication can be deactivated by setting this value to none. hmac-sha1-96 refers to the specifications in RFC-2404. hmac-sha2-256-128 refert to specifications in RFC-4868. Enumerations: none (0) hmac-sha1-96 (1) hmac-sha2-256-128 (2)
KeyVal
Octet-string (value) of secret shared with this Map-Server and used for Map-Register-authentication. Its length is internally padded/truncated to lispMapSrvKeyLen. Length: 0 to 255
KeyLen
Tells lispMapSrvKeyId-specific length for internally used copy of lispMapSrvKeyVal.
AuthMode
Tells for hmac-sha1-96 if authentication-data shall be stored in full 160-bits-length (skip-trunc-if-opt) or in truncated 96-bits-length (do-trunc-if-opt). RFC-6830 and RFC-2104 leave this choice open but some Map-Servers may support only one variant. For hmac-sha2-256-128, this setting has no effect because truncation to 128-bits-length is mandatory there. Enumerations: skip-trunc-if-opt (0) do-trunc-if-opt (1)
AuthLen
Tells lispMapSrvKeyId-specific and lispMapSrvAuthMode-specific length of authentication-data added to Map-Register-frames.

MIB Reference to Software Version 10.1.21 generated on 2016/12/23. Provided by webmaster@bintec-elmeg.com Copyright ©2016 by bintec elmeg GmbH