>> MIB - Management Information Base
>> Table: sysStat - (.1.3.6.1.4.1.272.4.17.500)
sysStat
OID | Name | Type | Access
.1 | BootConfig | ENUM | R
.2 | FunctionState | ENUM | R
.3 | OperationMode | ENUM | R
BootConfig
After system boot this variable shows which configuration was loaded: none: no configuration whatsoever bootfac: factory boot configuration default: default configuration as provided by image boot: configuration found in flash. Enumerations: none (1) bootfac (2) default (3) boot (4)
FunctionState
This variable contains the current function state, which is toggeled by pressing the function button on the device. Enumerations: on (1) off (2)
OperationMode
This variable defines the operation mode of the device concerning telephony functionality. If any voice functionality is integrated it can be either mgw(1) for Media GateWay functionality of pbx(2) for a full-fledged telephone system. For systems w/o voice functionality the variable has value plain(0). Enumerations: plain (0) mgw (1) pbx (2)

MIB Reference to Software Version 10.1.21 generated on 2016/12/23. Provided by webmaster@bintec-elmeg.com Copyright ©2016 by bintec elmeg GmbH