>> MIB - Management Information Base
>> Table: ip6DhcpStaticIfIdentTable - (.1.3.6.1.4.1.272.4.5.100.4.6.1)
Description: Interface-IDs (least significant 64 bits, see 2.5.1 of RFC-4291) for semi-statically assigned 'ip6DhcpClientAddress' entries (find more details on address-building there). Related DHCPv6-client is specified by 'ClientDUID' of related 'ip6DhcpOptionSet' entry. Warning: Clients with static interface-IDs do not get any other addresses than such ending with one of their specified interface-IDs, making any address-conflicts more critical. Additionally, if clients with static interface-IDs request multiple IAs on the same link because they have multiple interfaces to it, only the first IA will receive the related addresses.
ip6DhcpStaticIfIdentTable
OID | Name | Type | Access
.1 | Id | INTEGER | RW
.2 | AdminStatus | ENUM | D
.3 | Description | DisplayString | RW
.4 | OptionSetId | INTEGER | RW
.5 | Identifier | InetAddressIPv6 | RW
Id
Internal identifier of this static interface-ID-entry.
AdminStatus
Activate/deactivate/delete this static interface-ID-entry. Enumerations: enabled (1) disabled (2) delete (3)
Description
Textual description of this static interface-ID-entry. Length: 0 to 255
OptionSetId
'Id' value of related 'ip6DhcpOptionSet' entry. If no 'ip6DhcpOptionSetId' matches, this entry is ignored. 'ClientDUID' must be specified in related 'ip6DhcpOptionSet' entry in order to avoid that same address is assigned to multiple clients. Range: 1 to 65535
Identifier
Static interface-ID-value (see 2.5.1 of RFC-4291). Length: 16 to 16

MIB Reference to Software Version 10.1.21 generated on 2016/12/23. Provided by webmaster@bintec-elmeg.com Copyright ©2016 by bintec elmeg GmbH