>> MIB - Management Information Base
>> Table: mpsCallListTable - (.1.3.6.1.4.1.272.4.53.17.3.1)
Description: This table contains status information about each missed or normal terminated call.
mpsCallListTable
OID | Name | Type | Access
.1 | Type | ENUM | R
.2 | User | UserIndexOrZero | R
.3 | Direction | ENUM | R
.4 | Reason | ENUM | R
.5 | DateAndTime | Date | R
.6 | UserNumber | DisplayString | R
.7 | RemoteNumber | DisplayString | R
.8 | TrunkNumber | DisplayString | R
.9 | TrunkGroup | TrunkGroupIndexOrZero | R
.10 | AdminStatus | ENUM | D
Type
This variable defines the type of the call list entry: user-call: a user established or received this call. system-call: the PBX-system established or received this call. Enumerations: user-call (1) system-call (2)
User
Specifies the user who established or received the call. It contains the reference to mpsUserIndex in the mpsUserTable. Range: 0 to 65535
Direction
Defines if the call was an incoming or an outgoing call. Enumerations: incoming (1) outgoing (2)
Reason
Defines the reason why the call was put into the call list. Enumerations: failed (1) accepted (2)
DateAndTime
The date and time of the call setup. Range: 0 to -1
UserNumber
This is the user (extension) number of the call. Length: 0 to 4
RemoteNumber
This is the remote (intern or extern) number of the call: If mpsCallListDirection = outgoing this field contains the real dialled number by the user. If mpsCallListDirection = incoming and no number is stored indicates an anonymous call. Length: 0 to 32
TrunkNumber
This is the external trunk number (MSN or DDI) of the call. Length: 0 to 32
TrunkGroup
Specifies the trunk line via the call was established or received. It contains the reference to mpsTrunkGroupIndex in the mpsTrunkGroupTable. Range: 0 to 65535
AdminStatus
Just for MIB entry deletion. Enumerations: enabled (1) delete (2)

MIB Reference to Software Version 10.1.21 generated on 2016/12/23. Provided by webmaster@bintec-elmeg.com Copyright ©2016 by bintec elmeg GmbH