>> MIB - Management Information Base
>> Table: lispInstTable - (.1.3.6.1.4.1.272.4.23.9.1.1)
Description: List of configured LISP-instances (see section 5.5 of RFC-6830). With each LISP-instance, a corresponding entry is stored in ifTable and biboAdmDeviceTable.
lispInstTable
OID | Name | Type | Access
.1 | Id | INTEGER | RW
.2 | Index | InterfaceIndexOrZero | R
.3 | AdminStatus | ENUM | D
.4 | Descr | DisplayString | RW
.5 | Mtu | INTEGER | RW
.6 | CacheMaxSites | Unsigned32 | RW
.7 | CacheMaxEtrs | Unsigned32 | RW
.8 | CacheMaxFrames | Unsigned32 | RW
.9 | DefaultTtl | Unsigned32 | RW
.10 | ResolvingTtl | Unsigned32 | RW
.11 | DefTtlMode | ENUM | RW
.12 | ProxyEtrAddr | IpAddress | RW
Id
Identifier for this LISP-instance (see section 5.5 of RFC-6830). Special value of -1 identifies default-instance. In this case, Instance-ID-field is skipped in related LISP-frames. Remark: At most one default-LISP-instance may be specified. Range: -1 to 16777215
Index
Automatically selected index of virtual LISP-interface, stored as ifIndex in related ifTable-entry and stored as ipExtRtDstIfIndex in related ipExtRt-entries. Remark: Is set to zero if interface-selection fails. Range: 0 to 2147483647
AdminStatus
Administrative status of LISP-instance. Set to delete for killing entry. Enumerations: active (1) inactive (2) delete (3)
Descr
Optional name of LISP-instance, stored as ifDescr in related ifTable-entry. In case of empty string, ifDesc is set automatically. Length: 0 to 255
Mtu
Largest datagrams-size, stored as ifMtu in related ifTable-entry. Range: 1 to 8192
CacheMaxSites
Maximum number of stored lispCchSite entries for this LISP-instance.
CacheMaxEtrs
Maximum number of lispCchEtr entries stored per lispCchSite entry for this LISP-instance.
CacheMaxFrames
Maximum number of data-frames buffered per to-be-resolved lispCchEtr entry for this LISP-instance.
DefaultTtl
Default time-to-live in minutes for lispCchSite-entries of this LISP-instance. See description of lispInstDefTtlMode-field about when this default-value is used instead of the Map-Server-reported one.
ResolvingTtl
Time-to-live in minutes stored in lispCchSite entries that are still in to-be-resolved state for this LISP-instance.
DefTtlMode
Tells if lispInstDefaultTtl-field for this LISP-instance is used only as 'fallback' when Map-Server does not specify TTL, or if TTL is 'fixed' to this default-value (i.e. TTL from Map-Server is ignored). Enumerations: fallback (1) fixed (2)
ProxyEtrAddr
Optional Proxy-ETR-RLOC for special handling of negative Map-Replies with action 'Natively-Forward' (see section 6.1 of RFC-6832 and description of 'ACT' field in section 6.1.4 of RFC-6830). Per default, current LISP-implementation ignores action-parameter in negative Map-Replies and always assumes 'No-Action'. However, if this MIB-field is set (i.e. not 0.0.0.0) then it specifies Proxy-ETR-RLOC to be used for this LISP-instance for any target-EIDs resolved via negative Map-Reply with action 'Natively-Forward'.

MIB Reference to Software Version 10.1.21 generated on 2016/12/23. Provided by webmaster@bintec-elmeg.com Copyright ©2016 by bintec elmeg GmbH