>> MIB - Management Information Base
>> Table: bacAudioCodecPropertyTable - (.1.3.6.1.4.1.272.4.60.1.6.1)
Description: One entry in bacAudioCodecPropertyTable.
bacAudioCodecPropertyTable
OID | Name | Type | Access
.1 | Index | INTEGER | R
.2 | Descr | DisplayString | R
.3 | Bandwidth | INTEGER | R
.4 | FrameDuration | INTEGER | R
.5 | FrameSize | INTEGER | R
.6 | MosValue | INTEGER | R
Index
The id of the codec and index in this property table. Range: 1 to 32
Descr
The decription of this codec entry. Length: 0 to 255
Bandwidth
The required bandwidth in bits per seconds.
FrameDuration
The duration of one frame in microseconds.
FrameSize
The size of one frame in bits.
MosValue
The mean opinion score of this codec in hundredth. MOS specifies a numerical indication of the perceived audio quality. The following rating scheme exists: 1.00 Bad 2.00 Poor 3.00 Fair 4.00 Good 5.00 Excellent Range: 100 to 500

MIB Reference to Software Version 10.1.21 generated on 2016/12/23. Provided by webmaster@bintec-elmeg.com Copyright ©2016 by bintec elmeg GmbH