>> MIB - Management Information Base
>> Table: wlcAutoWTPTable - (.1.3.6.1.4.1.272.4.61.1.36.1)
Description: The table defines auto configuration of each WTP.
wlcAutoWTPTable
OID | Name | Type | Access
.1 | Index | INTEGER | RW
.2 | SelectorIndex | INTEGER | RW
.3 | Location | DisplayString | RW
.4 | Description | DisplayString | RW
.5 | secIndex | INTEGER | RW
.6 | localServicesIndex | INTEGER | RW
.7 | AdminStatus | ENUM | D
Index
Unique index.
SelectorIndex
Configured Selector index. See wlcAutoSelectorIndex.
Location
Location of the requested WTP. Length: 0 to 63
Description
Description of the requested WTP. Length: 0 to 63
secIndex
This attribute shows the currently configured secIndex of the requested WTP.
localServicesIndex
This attribute shows the currently configured localServicesIndex of the requested WTP.
AdminStatus
Delete the requested auto WTP. Enumerations: enabled (1) disabled (2) delete (3)

MIB Reference to Software Version 10.1.21 generated on 2016/12/23. Provided by webmaster@bintec-elmeg.com Copyright ©2016 by bintec elmeg GmbH