>> MIB - Management Information Base
>> Table: wlanPresenceServerTable - (.1.3.6.1.4.1.272.4.46.36.1)
Description: Contains all collection servers defined by the user.
wlanPresenceServerTable
OID | Name | Type | Access
.1 | Index | INTEGER | RW
.2 | Address | DisplayString | RW
.3 | Secret | DisplayString | RW
.4 | Validator | DisplayString | RW
.5 | RowStatus | ENUM | D
Index
Unique index of the server.
Address
Collection server address. The server address starts with 'http' or 'https', providing this last option security mechanisms, followed by an IP address or a domain name with an optional port number separated by a colon. An aditional resource address can be appended at the end of this field.
Secret
Secret string used by the collection server for accepting incoming messages.
Validator
Organization-specific validator string. The one provided by the collection server must match this one.
RowStatus
The row-status of a server entry.

MIB Reference to Software Version 10.1.21 generated on 2016/12/23. Provided by webmaster@bintec-elmeg.com Copyright ©2016 by bintec elmeg GmbH