>> MIB - Management Information Base
>> Table: mpsExtensionModeTable - (.1.3.6.1.4.1.272.4.53.6.12.1)
Description: This table contains the detailed information about extension modes.
mpsExtensionModeTable
OID | Name | Type | Access
.1 | Index | Unsigned32 | RW
.2 | ExtIndex | ExtensionIndex | RW
.3 | Mode | Unsigned32 | RW
.4 | ReRouteIndex | ReRouteIndexOrZero | RW
.5 | AdminStatus | ENUM | D
Index
A unique value for each mode for extension.
ExtIndex
Reference to the extension for this mode entry. Range: 1 to 65535
Mode
For each extension index can exist several mode entries. (One entry for each mode.)
ReRouteIndex
Index of the ReRouting function in mpsReRouteTable. 0 = ReRouting function inactive. Range: 0 to 65535
AdminStatus
Just for MIB entry deletion. Enumerations: enable (1) delete (2)

MIB Reference to Software Version 10.1.21 generated on 2016/12/23. Provided by webmaster@bintec-elmeg.com Copyright ©2016 by bintec elmeg GmbH