>> MIB - Management Information Base
>> Table: sTunnelAdm - (.1.3.6.1.4.1.272.4.38.12.1.1)
sTunnelAdm
OID | Name | Type | Access
.1 | Status | ENUM | RW
.2 | MaxTunnels | INTEGER | R
.3 | RunningTunnels | INTEGER | R
.4 | KeepAliveRetries | INTEGER | RW
.5 | KeepAliveTimeout | INTEGER | RW
Status
The AdminStatus of STunnel overall. This means if this Status is set to 'down' no tunnel will be established. So it doesn't matter if a single tunnel is set to AdminStatus 'down' or 'up'. In case of 'up' it depends on the single tunnel whether it is established or not. Enumerations: up (1) down (2)
MaxTunnels
The maximum of RUNNING tunnels in the system. Range: 0 to 65535
RunningTunnels
The number of running tunnels at the moment. Range: 0 to 65535
KeepAliveRetries
The maximum number of TCP keepalive retries sent before the (SSL) TCP connection is closed as it is suggested that the remote side isn't reachable anymore. The default value is 0 which takes the default number of retries of TCP. Range: 0 to 255
KeepAliveTimeout
The timeout (in seconds) of a TCP keepalive try. If no answer is received within this time another retry will be sent. The default value is 0 which takes the default keepalive retry timeout of TCP. Range: 0 to 65535

MIB Reference to Software Version 10.1.21 generated on 2016/12/23. Provided by webmaster@bintec-elmeg.com Copyright ©2016 by bintec elmeg GmbH