>> MIB - Management Information Base
>> Table: mpsCallListConfig - (.1.3.6.1.4.1.272.4.53.17.2)
mpsCallListConfig
OID | Name | Type | Access
.1 | AccountCalls | ENUM | RW
.2 | AccountAccepted | ENUM | RW
.3 | MaxUserEntries | INTEGER | RW
.4 | MaxSystemEntries | INTEGER | RW
.5 | SystemCount | Counter32 | R
AccountCalls
This value determines which calls are to be accounted. Enumerations: none (1) incoming-only (2) all (3)
AccountAccepted
Defines whether accepted (connected) calls should be accounted. If set to false only missed calls are collected. Enumerations: true (1) false (2)
MaxUserEntries
Maximum count of call list entries for each user. Range: 10 to 200
MaxSystemEntries
Maximum count of system call list entries. Range: 10 to 1000
SystemCount
Counter of current system call list entries.

MIB Reference to Software Version 10.1.21 generated on 2016/12/23. Provided by webmaster@bintec-elmeg.com Copyright ©2016 by bintec elmeg GmbH