>> MIB - Management Information Base
>> Table: mpsTrunkNumberUserTable - (.1.3.6.1.4.1.272.4.53.3.8.1)
Description: This table contains information about current mode for incoming call distribution to an immediately rerouting function.
mpsTrunkNumberUserTable
OID | Name | Type | Access
.1 | Index | TrunkNumberIndex | RW
.2 | Mode | Unsigned32 | RW
.3 | AdminStatus | ENUM | D
Index
A unique value for each trunk number, references mpsTrunkNumberIndex in mpsTrunkNumberTable. Range: 1 to 65535
Mode
This variable contains the actual mode for incoming call distribution to a reroute function.
AdminStatus
Just for MIB entry deletion. Enumerations: enable (1) delete (2)

MIB Reference to Software Version 10.1.21 generated on 2016/12/23. Provided by webmaster@bintec-elmeg.com Copyright ©2016 by bintec elmeg GmbH