>> MIB - Management Information Base
>> Table: ip6AdmRouteTable - (.1.3.6.1.4.1.272.4.5.100.1.5.1)
Description: A administrative routing entry.
ip6AdmRouteTable
OID | Name | Type | Access
.1 | Target | InetAddressIPv6 | RW
.2 | TargetLen | INTEGER | RW
.3 | Source | InetAddressIPv6 | RW
.4 | SourceLen | INTEGER | RW
.5 | IfIndex | InterfaceIndex | RW
.6 | NextHop | InetAddressIPv6 | RW
.7 | AdminStatus | ENUM | D
.8 | Priority | INTEGER | RW
.9 | Descr | DisplayString | RW
Target
The destination IPv6 address of this route. This object may not take a Multicast address value. Length: 16 to 16
TargetLen
Indicates the prefix length of the destination address. Range: 0 to 128
Source
The Source IPv6 address of this route. This object may not take a Multicast address value. Length: 16 to 16
SourceLen
Indicates the prefix length of the source address. Range: 0 to 128
IfIndex
The index value which uniquely identifies the local interface through which the next hop of this route should be reached. The interface identified by a particular value of this index is the same interface as identified by the same value of ip6DeviceIfIndex. For routes of the discard type this value can be zero. Range: 1 to 2147483647
NextHop
On remote routes, the address of the next hop, otherwise set to :: Length: 16 to 16
AdminStatus
The administrative status of this routing entry. Enumerations: enable (1) disable (2) delete (3)
Priority
The routing priority for this route, a value of 0 means highest priority, a value of 16 lowest priority. Range: 0 to 16
Descr
User defined description of this routing entry Length: 0 to 255

MIB Reference to Software Version 10.1.21 generated on 2016/12/23. Provided by webmaster@bintec-elmeg.com Copyright ©2016 by bintec elmeg GmbH