>> MIB - Management Information Base
>> Table: ipsecRadius - (.1.3.6.1.4.1.272.4.26.13)
ipsecRadius
OID | Name | Type | Access
.1 | PresetState | ENUM | R
.2 | PresetPeers | INTEGER | R
.3 | DynamicAuthentication | ENUM | RW
PresetState
This object shows the status of the RADIUS preset peers load process. Enumerations: not-loaded (1) loading (2) loaded (3) reloading (4)
PresetPeers
The number of RADIUS preset peers currently loaded.
DynamicAuthentication
This object enables/disables dynamic authentication via RADIUS. If no peer has been found matching an incoming IKE negotiation, the configured RADIUS servers are consulted (if any). Enumerations: enabled (1) disabled (2)

MIB Reference to Software Version 10.1.21 generated on 2016/12/23. Provided by webmaster@bintec-elmeg.com Copyright ©2016 by bintec elmeg GmbH