>> MIB - Management Information Base
>> Table: ip6DhcpClientFqdnOptTable - (.1.3.6.1.4.1.272.4.5.100.4.7.1)
Description: Statically assigned client-FQDNs (see 4 of RFC-4704). If router is configured as DNS-server then related (name, address) entries are added also into DNS-cache, independently from whether FQDN-option is requested or not. In case of FQDN-request, at most one entry may be replied. Thus, following rule applies. If entry with empty 'Name' matches and if client provides own name then it is simply confirmed. Otherwise, 'first' matching one is taken according to sorting-order defined via 'ip6DhcpClientFqdnOptListIdx'.
ip6DhcpClientFqdnOptTable
OID | Name | Type | Access
.1 | Id | INTEGER | RW
.2 | AdminStatus | ENUM | D
.3 | Description | DisplayString | RW
.4 | OptionSetId | INTEGER | RW
.5 | ListIdx | INTEGER | RW
.6 | Name | DisplayString | RW
.7 | FullName | DisplayString | R
Id
Internal identifier of this FQDN-entry.
AdminStatus
Activate/deactivate/delete this FQDN-entry. Enumerations: enabled (1) disabled (2) delete (3)
Description
Textual description of this FQDN-entry. Length: 0 to 255
OptionSetId
'Id' value of related 'ip6DhcpOptionSet' entry. If no 'ip6DhcpOptionSetId' matches, this FQDN-entry is ignored. 'ClientDUID' must be specified in related 'ip6DhcpOptionSet' entry in order to avoid that same FQDN is assigned to multiple clients. Range: 1 to 65535
ListIdx
Defines sorting-order in case of several matching FQDN-entries. Lower number means 'earlier in list'. Range: 0 to 255
Name
Fully qualified domain-name, or empty. If empty, 'Name' field of related 'ip6DhcpStatefulClient' is used instead, if not also empty. At most one entry with empty 'Name' should be specified per client. Fully qualified domain-names must have trailing dot for distinction from relative/partial domain-names. However, many users/admins tend to forget this. Thus, 'proper version' of this field is stored in field 'FullName'. Length: 0 to 255
FullName
'Proper' fully qualified domain-name, or empty. See description of field 'Name'. Length: 0 to 255

MIB Reference to Software Version 10.1.21 generated on 2016/12/23. Provided by webmaster@bintec-elmeg.com Copyright ©2016 by bintec elmeg GmbH