>> MIB - Management Information Base
>> Table: ipDns - (.1.3.6.1.4.1.272.4.5.20)
ipDns
OID | Name | Type | Access
.1 | DhcpAssign | ENUM | RW
.2 | IpcpAssign | ENUM | RW
.3 | UsePosCache | ENUM | RW
.4 | UseNegCache | ENUM | RW
.5 | MaxCacheSize | INTEGER | RW
.6 | PositiveTtl | INTEGER | RW
.7 | NegativeTtl | INTEGER | RW
.8 | DefaultIfIndex | INTEGER | RW
.9 | NumReceives | INTEGER | R
.10 | NumInvalids | INTEGER | R
.11 | NumRequests | INTEGER | R
.12 | NumCacheHits | INTEGER | R
.13 | NumForwards | INTEGER | R
.14 | NumOks | INTEGER | R
.15 | NumFails | INTEGER | R
.17 | DynamicGlobals | ENUM | RW
DhcpAssign
Assignment policy when a BinTec router acts as a DHCP-server and is asked for nameserver addresses. Possible values: - none: Do not send any nameserver-addresses. - self: Send own address as the only nameserver. - global: Send addresses from global nameserver-table. Enumerations: none (1) self (2) global (3)
IpcpAssign
Assignment policy when a BinTec router is asked for nameservers during IPCP negotiation. Possible values: - none: Do not send any nameserver addresses. - self: Send own address as the only nameserver. - global: Send addresses from global namerserver-table. Enumerations: none (1) self (2) global (3)
UsePosCache
Decides whether positive dynamic caching is done or not. Enumerations: no (1) yes (2)
UseNegCache
Decides whether negative dynamic caching is done or not. Enumerations: no (1) yes (2)
MaxCacheSize
Defines maximum number of dynamic DNS-table-entries. If this limit is reached, the least recently used dynamic entry is discarded if a new one is to be added.
PositiveTtl
Time-to-live in seconds reported for positive static entries.
NegativeTtl
Time-to-live in seconds reported for negative static entries, and initial time-to-live for negative dynamic cache-entries.
DefaultIfIndex
Interface-index (if not -1) of DHCP/IPCP-assigned nameserver that should be used as fallback for DNS-forwarding if not found by other mechanism (e.g. manually configured global nameserver or address/interface specified by application or wildcard-domain-forwarding-entry).
NumReceives
The number of packets received.
NumInvalids
The number of invalid packets received.
NumRequests
The number of questions received. If a packet is received, this variable is incremented by the number of question records contained in the packet.
NumCacheHits
The number of times a question could be answered immediately due to a cache entry.
NumForwards
The number of questions forwarded to other nameservers.
NumOks
The number of requests answered successfully.
NumFails
The number of requests answered with a SERVFAIL packet.
DynamicGlobals
Determines if 'automatic' entries (see ipDnsServerCfgMode) are stored in global nameserver-table: - yes: Make 'automatic' nameserver-entries. - no: Do NOT make 'automatic' nameserver-entries. Enumerations: yes (1) no (2)

MIB Reference to Software Version 10.1.21 generated on 2016/12/23. Provided by webmaster@bintec-elmeg.com Copyright ©2016 by bintec elmeg GmbH