>> MIB - Management Information Base
>> Table: systemPhoneFwuFileTable - (.1.3.6.1.4.1.272.4.64.5.2.1)
Description: This entries only created by the respective device driver.
systemPhoneFwuFileTable
OID | Name | Type | Access
.1 | Index | INTEGER | RW
.2 | Type | ENUM | RW
.3 | Directory | DisplayString | RW
.4 | Name | DisplayString | RW
.5 | Version | DisplayString | RW
.6 | AdminStatus | ENUM | D
Index
A counting index for each firmware file stored on the mounted device. Range: 1 to 65535
Type
Variable contains the phone type of firmware file (stripped out of the header of the file). Enumerations: cs290 (20) cs410 (22) cs290u (23) cs410u (24) cs400 (25) ips290 (32) ips400 (33) ips290plus (34) s530 (64) s560 (65) ost-40 (144) ost-80 (145) ip120 (160) ip140 (161) dect150 (162) dect200-b (163) dect200-m (164) ip130 (165) ip620 (166) ip630 (168) ip680 (171) de310-ip-pro (176) de410-ip-pro (177) de700-ip-pro (178) de900-ip-pro (179) n510-ip-pro (180) n720-ip-pro (181) n720-dm-pro (182) maxwell-basic (183) maxwell-3 (185) maxwell-10 (188)
Directory
Specifies the complete path/tree where the firmware file can be found on the mounted device. Length: 0 to 255
Name
Simply contains the firmware file name on the mounted device. Length: 0 to 255
Version
Version information of the firmware file stored on sd card (stripped out of the header of file). Version string of elmeg system phones have a size of max. 9 characters. Siemens OpenStage devices have a maximum size of 12. Length: 0 to 20
AdminStatus
Just for MIB entry deletion. Enumerations: enable (1) delete (2)

MIB Reference to Software Version 10.1.21 generated on 2016/12/23. Provided by webmaster@bintec-elmeg.com Copyright ©2016 by bintec elmeg GmbH