>> MIB - Management Information Base
>> Table: systemPhoneFwuServer - (.1.3.6.1.4.1.272.4.64.5.1)
systemPhoneFwuServer
OID | Name | Type | Access
.1 | StartHour | INTEGER | RW
.2 | StartMinute | INTEGER | RW
.3 | EndHour | INTEGER | RW
.4 | EndMinute | INTEGER | RW
.5 | FileStatus | ENUM | RW
.6 | UploadResult | ENUM | R
.7 | UploadStatus | ENUM | R
.8 | RemoteAccessAllowed | ENUM | RW
.9 | UrlAllowed | ENUM | RW
StartHour
Every day firmware update start time (hour). Range: 0 to 24
StartMinute
Every day firmware update start time (minute). Range: 0 to 60
EndHour
Every day firmware update end time (hour). Range: 0 to 24
EndMinute
Every day firmware update end time (minute). Range: 0 to 60
FileStatus
Firmware file status: create(1): new firmware file shall be stored on the device done(2): synchronization of storage device with MIB is done. Enumerations: create (1) done (2)
UploadResult
Firmware file upload result (error) code: success(1): the firmware file upload was successful, no-mem-card(2): no memory card plugged in, no-mem-space(3): no more space available on the memory card, incomp-fw-format(4): the firmware file format doesn't match the requirements, transfer-error(5): any transfer error occured during upload, write-protection(6): active write protection on storage device, internal-error(7): unexpected internal error occured. Enumerations: success (1) no-mem-card (2) no-mem-space (3) incomp-fw-format (4) transfer-error (5) write-protection (6) internal-error (7)
UploadStatus
Firmware file upload status: progress(1): firmware file storage on the device is in progress, done(2): firmware file storage on the device and synchronization with MIB is done. Enumerations: progress (1) done (2)
RemoteAccessAllowed
Allow/block access to the intern FW-UPD Server from extern ISDN. Enumerations: true (1) false (2)
UrlAllowed
Allow/block access to extern FW-UPD Server (URL) from intern (e. g. Gigaset Maxwell Series) phone devices. Enumerations: true (1) false (2)

MIB Reference to Software Version 10.1.21 generated on 2016/12/23. Provided by webmaster@bintec-elmeg.com Copyright ©2016 by bintec elmeg GmbH