>> MIB - Management Information Base
>> Table: mdmTable - (.1.3.6.1.4.1.272.4.18.2.1)
Description: The mdmTable contains information for each modem. The entries contain various statistical data for modem connections. Only the system can add entries to this table. The user is able to reboot, enable or disable a modem. The system updates infos about the current connection.
mdmTable
OID | Name | Type | Access
.1 | Index | INTEGER | R
.2 | Action | ENUM | RW
.3 | Type | ENUM | R
.4 | State | ENUM | R
.5 | Mode | ENUM | R
.6 | Modulation | ENUM | R
.7 | ErrorCorr | ENUM | R
.8 | Compression | ENUM | R
.9 | XmitSpeed | INTEGER | R
.10 | RcvSpeed | INTEGER | R
.11 | IfIndex | INTEGER | R
.12 | IfBchannel | INTEGER | R
Index
Index of this modem (Slot/Cpu/Modem)
Action
Writing to this variable reboot (1) : initiates a reboot. disabled (2) : remove modem resource from allocation pool. enabled (3) : put modem to allocation resource pool. Enumerations: reboot (1) disabled (2) enabled (3)
Type
Type of this modem csm56K (1) : CentralSiteModem K56Flex csm336 (2) : CentralSiteModem 33600 mdm144 (3) : ClientSiteModem 14400 mdm336 (4) : ClientSiteModem 33600 telindus (5) : ADSP with Telindus firmware Enumerations: csm56K (1) csm336 (2) mdm144 (3) mdm336 (4) telindus (5)
State
Current status of the modem. booting (1) : init phase idle (2) : this modem resource is available calling (3) : outgoing call initiated called (4) : incoming call initiated connected (5) : data transfer phase established hangup (6) : going to terminate a connection stopped (7) : out of order, modem ist not useable Enumerations: booting (1) idle (2) calling (3) called (4) connected (5) hangup (6) stopped (7)
Mode
Type of mode modem (1) : modem native ppp (2) : modem native + async hdlc fax (3) : fax mode dtmf (4) : receive and signal DTMF touchtones voice (5) : support various VoIP modes none (7) : modem curently not used Enumerations: modem (1) ppp (2) fax (3) dtmf (4) voice (5) none (7)
Modulation
Negotiated modulation. same as mdmProfileModulation. Enumerations: bell103 (1) bell212 (2) v21 (3) v22 (4) v22bis (5) v23 (6) v32 (7) v32bis (8) v34 (9) k56flex (10) vfc (11) v90 (12) unknown (31)
ErrorCorr
Negotiated error correction protocol. none (1) : no error correction alt (2) : MNP error correction established lapm (3) : LAPM error correction established Enumerations: none (1) alt (2) lapm (3)
Compression
Negotiated compression correction protocol. none (1) : no compression class5 (2) : MNP5 compression v42bis (3) : V.42bis compression Enumerations: none (1) class5 (2) v42bis (3)
XmitSpeed
Negotiated transmit speed.
RcvSpeed
Negotiated receive speed.
IfIndex
the (ISDN) interface's slot this modem is connected to
IfBchannel
the (ISDN) interface's B channel this modem is connected to Range: 0 to 31

MIB Reference to Software Version 10.1.21 generated on 2016/12/23. Provided by webmaster@bintec-elmeg.com Copyright ©2016 by bintec elmeg GmbH