>> MIB - Management Information Base
>> Table: ipsecInternalSubnetTable - (.1.3.6.1.4.1.272.4.26.34.1)
Description: Lists to-be-reported attributes of type INTERNAL_IP4_SUBNET or INTERNAL_IP6_SUBNET (see section 3.15.2 of RFC-7296). Traffic-selector-negotiation or child-SA-allocation are NOT affected by these entries. Entries are relevant for IKEv2 only.
ipsecInternalSubnetTable
OID | Name | Type | Access
.1 | PeerIndex | INTEGER | RW
.2 | Description | DisplayString | RW
.3 | AddressType | ENUM | RW
.4 | Address | InetAddress | RW
.5 | PrefixLength | InetAddressPrefixLength | RW
.6 | AdminStatus | ENUM | D
PeerIndex
Index of ipsecPeer that shall be informed about this subnet.
Description
Optional human-readable description for this entry. Length: 0 to 255
AddressType
Fields (AddressType, Address, PrefixLength) specify subnet for this entry. At present, following address-types are allowed: ipv4 -- Entry specifies INTERNAL_IP4_SUBNET attribute. Allowed PrefixLength range is [0..32]. ipv6 -- Entry specifies INTERNAL_IP6_SUBNET attribute. Allowed PrefixLength range is [0..128]. Any other values implicitly invalidate this entry. Enumerations: unknown (0) ipv4 (1) ipv6 (2) ipv4z (3) ipv6z (4) dns (16)
Address
See description of AddressType field. Length: 0 to 255
PrefixLength
See description of AddressType field. Range: 0 to 2040
AdminStatus
Activate/deactivate/delete this entry. Enumerations: enabled (1) disabled (2) delete (3)

MIB Reference to Software Version 10.1.21 generated on 2016/12/23. Provided by webmaster@bintec-elmeg.com Copyright ©2016 by bintec elmeg GmbH