>> MIB - Management Information Base
>> Table: voipStatCallTable - (.1.3.6.1.4.1.272.4.33.22.2.1)
Description: Describes the call statistics for a SIP account.
voipStatCallTable
OID | Name | Type | Access
.1 | Index | INTEGER | R
.2 | Provider | INTEGER | R
.3 | Address | INTEGER | R
.4 | Action | ENUM | RW
.5 | LastReset | Date | R
.6 | Count | Counter32 | R
.7 | OutAttempt | Counter32 | R
.8 | OutAnswered | Counter32 | R
.9 | OutConnect | Counter32 | R
.10 | OutFailed | Counter32 | R
.11 | InReceive | Counter32 | R
.12 | InAnswered | Counter32 | R
.13 | InConnect | Counter32 | R
.14 | InFailed | Counter32 | R
.15 | Dropped | Counter32 | R
.16 | TotalConnectTime | INTEGER | R
.17 | ServerDownTime | INTEGER | R
.18 | TxPackets | Counter64 | R
.19 | TxBytes | Counter64 | R
.20 | RxPackets | Counter64 | R
.21 | RxBytes | Counter64 | R
Index
Unique Index value of this Entry
Provider
Reference to the SIP Account the statistic belongs.
Address
Reference to the subscriber Number of the concerning SIP Account.
Action
Reset all Statistic values to zero. done - reset executed reset - reset request Enumerations: done (1) reset (2)
LastReset
Date and time of last reset Range: 0 to -1
Count
Total number of calls (incoming and outgoing) including also not successfully completed calls
OutAttempt
Total attempted outgoing calls.
OutAnswered
Total outgoing calls answered.
OutConnect
Total outgoing successfully completed calls.
OutFailed
Total outgoing not successfully completed calls.
InReceive
Total incoming calls received
InAnswered
Total incoming calls signalled to the local user.
InConnect
Total incoming calls that successfully completed call setup signaling.
InFailed
Total incoming calls that failed to successfully complete call setup signaling.
Dropped
Total calls that were successfully connected (incoming or outgoing), but dropped unexpectedly while in progress without explicit user termination.
TotalConnectTime
Cumulative call connected duration in seconds.
ServerDownTime
The number of seconds the CPE is unable to maintain a connection to the server not including time in which overall network connectivity is unavailable. Applies only to SIP.
TxPackets
Total number of RTP packets sent for this line.
TxBytes
Total number of RTP payload bytes sent for this line.
RxPackets
Total number of RTP packets received for this line.
RxBytes
Total number of RTP payload bytes received for this line.

MIB Reference to Software Version 10.1.21 generated on 2016/12/23. Provided by webmaster@bintec-elmeg.com Copyright ©2016 by bintec elmeg GmbH