>> MIB - Management Information Base
>> Table: lispLocSiteTable - (.1.3.6.1.4.1.272.4.23.9.3.1)
Description: List of local LISP-sites (see section 4.2 of RFC-6833). For each pair of remote and local site of same LISP-instance, a corresponding entry is stored in ipExtRtTable.
lispLocSiteTable
OID | Name | Type | Access
.1 | InstId | INTEGER | RW
.2 | Addr | IpAddress | RW
.3 | Len | INTEGER | RW
.4 | Aligned | IpAddress | R
.5 | AdminStatus | ENUM | D
.6 | Ttl | Unsigned32 | RW
.7 | IfIndex | InterfaceIndexOrZero | RW
.8 | Metric1 | INTEGER | RW
.9 | RlocMode | ENUM | RW
InstId
Refers to lispInstId-field of related lispInst-entry. Range: -1 to 16777215
Addr
Together with lispLocSiteLen, specifies EID-prefix of this local LISP-site. Prefix is reported to configured Map-Servers via Map-Register.
Len
See description of lispLocSiteAddr. Converted/stored as ipExtRtSrcMask in related ipExtRt-entries. Range: 0 to 32
Aligned
Prefix-length-aligned read-only-version of lispLocSiteAddr. Stored as ipExtRtSrcAddr in related ipExtRt-entry.
AdminStatus
Administrative status of local LISP-site. Set to delete for killing entry. Enumerations: active (1) inactive (2) delete (3)
Ttl
Time-to-live-value in minutes that is reported via Map-Register for this local LISP-site.
IfIndex
Optional interface-index of this local LISP-site, stored as ipExtRtSrcIfIndex in related ipExtRt-entries. At present, it is not possible to assign multiple ifindex-values to the same local site. Special value of 0 means that interface-index is not specified. Range: 0 to 2147483647
Metric1
Stored as ipExtRtMetric1 in related ipExtRt-entries.
RlocMode
Tells how to fill reported ETR-RLOCs-list for this local LISP-site. Negative mappings have an empty ETR-RLOCs-list, i.e. matching frames cannot be LISP-tunnelled. The reported action-field for such mappings is currently hard-coded to 0 (i.e. drop matching frames silently). In automatic mode, ETR-RLOCs-list is auto-filled, based on current route/address-info. At present, ETR-RLOCs cannot be configured manually. Enumerations: negative (1) auto (2)

MIB Reference to Software Version 10.1.21 generated on 2016/12/23. Provided by webmaster@bintec-elmeg.com Copyright ©2016 by bintec elmeg GmbH