>> MIB - Management Information Base
>> Table: dot11SpectrumManagementTable - (.1.2.840.10036.1.8.1)
Description: An entry (conceptual row) in the Spectrum Management Table. IfIndex - Each 802.11 interface is represented by an ifEntry. Interface tables in this MIB are indexed by ifIndex.
dot11SpectrumManagementTable
OID | Name | Type | Access
.1 | SpectrumManagementIndex | Integer32 | R
.2 | MitigationRequirement | Integer32 | RW
.3 | ChannelSwitchTime | Integer32 | RW
.4 | PowerCapabilityMax | Integer32 | R
.5 | PowerCapabilityMin | Integer32 | R
SpectrumManagementIndex
The auxiliary variable used to identify instances of the columnar objects in the Spectrum Management Table. Range: 1 to 2147483647
MitigationRequirement
This attribute shall indicate the mitigation requirement in dB required. The default value of this attribute shall be 3 dB.
ChannelSwitchTime
This attribute shall indicate assumed channel switch time, measured in TUs. The unit of this attribute is TUs. The default value of this attribute shall be 2 TUs. The minimum value shall be 1 TU.
PowerCapabilityMax
This attribute shall indicate the maximum transmit Power Capability of this station. The unit of this attribute is dBm. The default value of this attribute shall be 0 dBm.
PowerCapabilityMin
This attribute shall indicate the minimum transmit Power Capability of this station. The unit of this attribute is dBm. The default value of this attribute shall be -100 dBm.

MIB Reference to Software Version 10.1.21 generated on 2016/12/23. Provided by webmaster@bintec-elmeg.com Copyright ©2016 by bintec elmeg GmbH