>> MIB - Management Information Base
>> Table: igmpStaticGroupTable - (.1.3.6.1.4.1.272.4.5.51.6.1)
Description: An entry (conceptual row) representing an statically connected member on an interface.
igmpStaticGroupTable
OID | Name | Type | Access
.1 | IfIndex | InterfaceIndex | RC
.2 | Address | IpAddress | RC
.3 | Status | ENUM | D
IfIndex
The ifIndex value of the static group. Range: 1 to 2147483647
Address
The group address of this entry.
Status
Status of this static group. Enumerations: active (1) notInService (2) notReady (3) createAndGo (4) createAndWait (5) destroy (6)

MIB Reference to Software Version 10.1.21 generated on 2016/12/23. Provided by webmaster@bintec-elmeg.com Copyright ©2016 by bintec elmeg GmbH