>> MIB - Management Information Base
>> Table: ip6DhcpPrefixPoolTable - (.1.3.6.1.4.1.272.4.5.100.4.5.1)
Description: DHCPv6-prefix-pools for filling requested IA_PD options (see 9 and 10 of RFC-3633).
ip6DhcpPrefixPoolTable
OID | Name | Type | Access
.1 | Id | INTEGER | RW
.2 | AdminStatus | ENUM | D
.3 | Description | DisplayString | RW
.4 | OptionSetId | INTEGER | RW
.5 | PrefixId | INTEGER | RW
.6 | SubPrefixLength | INTEGER | RW
.7 | StartOffset | InetAddressIPv6 | RW
.8 | StartPrefix | InetAddressIPv6 | R
.9 | EndOffset | InetAddressIPv6 | RW
.10 | EndPrefix | InetAddressIPv6 | R
.11 | Size | Counter64 | R
.12 | PrefLifetime | Unsigned32 | RW
.13 | ValidLifetime | Unsigned32 | RW
.14 | AutoRoutePrio | INTEGER | RW
.15 | OpPrefLifetime | Unsigned32 | R
.16 | OpValidLifetime | Unsigned32 | R
Id
Internal identifier of this prefix-pool.
AdminStatus
Activate/deactivate/delete this prefix-pool. Enumerations: enabled (1) disabled (2) delete (3)
Description
Textual description of this prefix-pool. Length: 0 to 255
OptionSetId
'Id' value of related 'ip6DhcpOptionSet' entry. If no 'ip6DhcpOptionSetId' matches, this prefix-pool is ignored. Range: 1 to 65535
PrefixId
'Id' value of related 'ip6Prefix' entry. Prefixes from this pool are assigned only if related 'ip6Prefix' entry exists and if its 'OperStatus' is not 'down'. If multiple pools refer to same 'ip6Prefix' then their ranges must not overlap (see 'ip6DhcpPrefixPoolStartOffset' and 'ip6DhcpPrefixPoolEndOffset'). If any 'ip6LinkPrefix' entries refer to same 'ip6Prefix' then their sub-prefixes must not overlap with prefix-range of this pool. 'IfIndex' of related 'ip6Prefix' entry must be zero (unspecified) because DHCPv6-clients may freely link-assign their prefixes. 'OnLinkFlag' of related 'ip6LinkPrefix' entry must be 'false'. 'AutonomousFlag' of related 'ip6LinkPrefix' entry must be 'false'.
SubPrefixLength
Length of generated sub-prefixes, must be <= 64 and >= related 'ip6PrefixLength'. Range: 0 to 64
StartOffset
Together with 'Prefix' of related 'ip6Prefix' entry, specifies lowest assignable prefix in this pool. Result of prefix plus offset is stored in 'StartPrefix' field. Lowest (128-'SubPrefixLength') bits of offset must be zero. Offset must be smaller than 2^(128-L) where L is 'Length' of related 'ip6Prefix' entry. Length: 16 to 16
StartPrefix
Lowest assignable prefix in this pool, or 0 if no suitable 'ip6Prefix' entry was found. See description of 'StartOffset' field for further details. Length: 16 to 16
EndOffset
Together with 'Prefix' of related 'ip6Prefix' entry, specifies highest assignable prefix in this pool. Result of prefix plus offset is stored in 'EndPrefix' field. Lowest (128-'SubPrefixLength') bits of offset must be zero. Offset must be smaller than 2^(128-L) where L is 'Length' of related 'ip6Prefix' entry. Offset must not be smaller than related 'StartOffset'. Length: 16 to 16
EndPrefix
Highest assignable prefix in this pool, or 0 if no suitable 'ip6Prefix' entry was found. See description of 'EndOffset' field for further details. Length: 16 to 16
Size
Number of prefixes in this pool, calculated by formula 1+(('EndPrefix'-'StartPrefix')/(2^(128-'SubPrefixLength'))), or 0 if no suitable 'ip6Prefix' entry was found. Warning: Due to 64-bit-restriction of this field, the maximum possible pool-size of 2^64 is also represented by a 0 value.
PrefLifetime
Maximum 'preferred lifetime' in seconds of prefixes in this pool. More details are described for 'ip6DhcpPrefixPoolOpPrefLifetime'.
ValidLifetime
Maximum 'valid lifetime' in seconds of prefixes in this pool. More details are described for 'ip6DhcpPrefixPoolOpValidLifetime'.
AutoRoutePrio
'Priority' value of related, auto-generated 'ip6AdmRoute' entries. A value of -1 means NO auto-generated 'ip6AdmRoute' entries. See also description for 'ip6DhcpClientPrefixFwdIfIndex' and 'ip6DhcpClientPrefixFwdAddress'. Range: -1 to 16
OpPrefLifetime
'Preferred lifetime' in seconds of prefixes in this pool (see 10 of RFC-3633). Value is set to minimum of configured maximum 'ip6DhcpPrefixPoolPrefLifetime' and inherited 'ip6PrefixAdvPreferredLifetime'.
OpValidLifetime
'Valid lifetime' in seconds of prefixes in this pool (see 10 of RFC-3633). Value is set to minimum of configured maximum 'ip6DhcpPrefixPoolValidLifetime' and inherited 'ip6PrefixAdvValidLifetime'.

MIB Reference to Software Version 10.1.21 generated on 2016/12/23. Provided by webmaster@bintec-elmeg.com Copyright ©2016 by bintec elmeg GmbH