>> MIB - Management Information Base
>> Table: biboPPPStatTable - (.1.3.6.1.4.1.272.4.3.2.1)
Description: The biboPPPStatTable contains statistical connection- specific information. Only the system can add or delete entries to this table. Creating entries: Entries are created by the system each time a new PPP interface is created in the biboPPPTable. Deleting entries: Entries are removed by the system when the corresponding PPP interface is removed.
biboPPPStatTable
OID | Name | Type | Access
.1 | ConnIfIndex | INTEGER | R
.2 | ConnActive | INTEGER | R
.3 | ConnProtocols | INTEGER | R
.4 | ConnState | ENUM | R
.5 | ConnDuration | INTEGER | R
.6 | ConnUnits | Counter | R
.7 | ConnTransmitOctets | Counter | R
.8 | ConnReceivedOctets | Counter | R
.9 | ConnOutgoingCalls | Counter | R
.10 | ConnOutgoingFails | Counter | R
.11 | ConnIncomingCalls | Counter | R
.12 | ConnIncomingFails | Counter | R
.13 | TotalDuration | INTEGER | R
.14 | TotalUnits | Counter | R
.15 | TotalTransmitOctets | Counter | R
.16 | TotalReceivedOctets | Counter | R
.17 | TotalOutgoingCalls | Counter | R
.18 | TotalOutgoingFails | Counter | R
.19 | TotalIncomingCalls | Counter | R
.20 | TotalIncomingFails | Counter | R
.21 | Throughput | Counter | R
.23 | ChargeInterval | INTEGER | R
.24 | IdleTime | INTEGER | R
.25 | ConnCharge | Counter | R
.26 | TotalCharge | Counter | R
.27 | LastConnDuration | INTEGER | R
.28 | LastConnIdle | INTEGER | R
ConnIfIndex
Correlating PPP interface index.
ConnActive
The actual number of bundled channels. Range: 1 to 250
ConnProtocols
The bitwise ORed protocols successfully negotiated on this connection; currently the following protocols are supported: tcp/ip(1), ipx(2), bridge(4), bpdu(8), x25(16). These protocol values are most likely to change in future software releases.
ConnState
The physical state of the link. This field is obsolete and will not be supported in a future release. Enumerations: idle (1) incoming (2) outgoing (3) connected (4) dataxfer (5) disconnect (6) authentication-failed (7) authentication-successful (8)
ConnDuration
The current link duration on this interface in seconds.
ConnUnits
The current costs on this interface for all member links.
ConnTransmitOctets
The octets transmitted on this interface since its last change to the 'up' state.
ConnReceivedOctets
The octets received since its last change to the `up' state.
ConnOutgoingCalls
The number of outgoing calls on this interface since its last change to the 'up' state.
ConnOutgoingFails
The number of outgoing call failures on this interface since its last change to the 'up' state.
ConnIncomingCalls
The number of incoming calls on this interface since its last change to the up state.
ConnIncomingFails
The number of incoming call failures on this interface since its last change to the up state.
TotalDuration
The total link duration in seconds.
TotalUnits
The total costs on this interface for all member links.
TotalTransmitOctets
The total amount of octets transmitted.
TotalReceivedOctets
The total amount of octets received.
TotalOutgoingCalls
The total number of outgoing calls.
TotalOutgoingFails
The total number of outgoing call failures.
TotalIncomingCalls
The total number of incoming calls.
TotalIncomingFails
The total number of incoming call failures.
Throughput
The actual throughput of the interface; updated every 5 seconds. Note that only the actual maximum of the both directions (send / receive) is considered.
ChargeInterval
Describes the measured interval between charging info elements received from the ISDN network. Range: 0 to 3600
IdleTime
The currently measured connection inactivity time (channel is silent). Range: 0 to 3600
ConnCharge
The current charge on this interface as 1/1000 of the respective currency.
TotalCharge
The total charge on this interface as 1/1000 of the respective currency.
LastConnDuration
The duration of the last connection on this interface in seconds.
LastConnIdle
The inactivity time of the last connection on this interface in seconds.

MIB Reference to Software Version 10.1.21 generated on 2016/12/23. Provided by webmaster@bintec-elmeg.com Copyright ©2016 by bintec elmeg GmbH