>> MIB - Management Information Base
>> Table: ip6DhcpDnsServerOptTable - (.1.3.6.1.4.1.272.4.5.100.4.9.1)
Description: Statically assigned recursive name-servers (see 3 of RFC-3646). If multiple entries match then all related addresses are stored in a single DNS-server-option according to sorting-order specified via 'ip6DhcpDnsServerOptListIdx'. If DNS-option is requested but no static entries match then rules of related 'ip6AdmIfDnsAssign' entry apply.
ip6DhcpDnsServerOptTable
OID | Name | Type | Access
.1 | Id | INTEGER | RW
.2 | AdminStatus | ENUM | D
.3 | Description | DisplayString | RW
.4 | OptionSetId | INTEGER | RW
.5 | ListIdx | INTEGER | RW
.6 | Address | InetAddressIPv6 | RW
Id
Internal identifier of this DNS-entry.
AdminStatus
Activate/deactivate/delete this DNS-entry. Enumerations: enabled (1) disabled (2) delete (3)
Description
Textual description of this DNS-entry. Length: 0 to 255
OptionSetId
'Id' value of related 'ip6DhcpOptionSet' entry. If no 'ip6DhcpOptionSetId' matches, this DNS-entry is ignored. Range: 1 to 65535
ListIdx
Defines sorting-order in case of several matching DNS-entries. Lower number means 'earlier in list'. Range: 0 to 255
Address
Address of DNS-server. Length: 16 to 16

MIB Reference to Software Version 10.1.21 generated on 2016/12/23. Provided by webmaster@bintec-elmeg.com Copyright ©2016 by bintec elmeg GmbH