>> MIB - Management Information Base
>> Table: ip6DsLiteTable - (.1.3.6.1.4.1.272.4.5.100.1.9.1)
Description: Contains a DsLite (4in6) configuration.
ip6DsLiteTable
OID | Name | Type | Access
.1 | IfIndexV4 | InterfaceIndexOrZero | RW
.2 | IfIndexV6 | InterfaceIndex | RW
.3 | Descr | DisplayString | RW
.4 | ConfigMode | ENUM | D
.5 | Encapsulation | ENUM | RW
.6 | LocalAddress | InetAddressIPv6 | RW
.7 | RemoteAddress | InetAddressIPv6 | RW
.8 | UsedLocalAddress | InetAddressIPv6 | R
.9 | UsedRemoteAddress | InetAddressIPv6 | R
IfIndexV4
Unique Identifier for this entry Range: 0 to 2147483647
IfIndexV6
Specifies the associated IPv6 interface for this entry. Range: 1 to 2147483647
Descr
Description for the DsLite connection Length: 0 to 255
ConfigMode
Configuration mode of the tunnel addresse. Enumerations: static (1) dhcp (2) delete (8)
Encapsulation
The encapsulation used for this tunnel. Enumerations: ipip (1) none (16)
LocalAddress
Static configured local IPv6 address of ithis tunnel. Length: 16 to 16
RemoteAddress
DsLite tunnel endpoint IPv6 address. Length: 16 to 16
UsedLocalAddress
Used local IPv6 address of this tunnel. Length: 16 to 16
UsedRemoteAddress
Used tunnel endpoint IPv6 address of this tunnel. Length: 16 to 16

MIB Reference to Software Version 10.1.21 generated on 2016/12/23. Provided by webmaster@bintec-elmeg.com Copyright ©2016 by bintec elmeg GmbH