>> MIB - Management Information Base
>> Table: pppoeAcTable - (.1.3.6.1.4.1.272.4.24.3.1)
Description: The pppoeAcTable is used to enable the PPPoE server mode (Access Concentrator) on the associated Ethernet interface. Creating entries: Entries are added by the user. Deleting entries: Entries are removed once the respective variable pppoeAcChkService is set to delete(4).
pppoeAcTable
OID | Name | Type | Access
.1 | EthIfIndex | INTEGER | RW
.2 | ChkService | ENUM | D
.3 | Name | DisplayString | RW
EthIfIndex
The interface index (ifIndex) of the associated Ethernet interface.
ChkService
If set to accept-all(1) this variable determines that - regardless of the PPPoE 'SERVICE-NAME' tag (see RFC 2516) - all PPPoE Active Discovery Initiation (PADI) packets will be accepted and answered with a PPPoE Active Discovery Offer (PADO) packet. If set to accept-from-list(2) only PADI packets with a 'SERVICE-NAME' tag matching with one of the services specified via the pppoeAcServiceTable will be accepted and answered. If set to delete(4), this entry will be removed and PADI packets received on the associated Ethernet interface will be ignored. Enumerations: accept-all (1) accept-from-list (2) delete (4)
Name
The PPPoE AC-NAME to be used for PPPoE Active Discovery Offer (PADO) and PPPoE Active Discovery Session-confirmation (PADS) packet. If not specified, the given system name (sysName) will be used as fallback. Length: 0 to 255

MIB Reference to Software Version 10.1.21 generated on 2016/12/23. Provided by webmaster@bintec-elmeg.com Copyright ©2016 by bintec elmeg GmbH