>> MIB - Management Information Base
>> Table: ip6DhcpClientAddressTable - (.1.3.6.1.4.1.272.4.5.100.4.12.1)
Description: Currently assigned client-addresses, built for each pair of requested IA_NA and matching 'ip6LinkPrefix' entry. For clients with semi-statically assigned addresses, the interface-ID part (least significant 64 bits, see section 2.5.1 of RFC-4291) is taken from their 'ip6DhcpStaticIfIdent' entries. For all other clients, some random interface-ID (excluding any static ones) is used unless they request some specific and valid addresses.
ip6DhcpClientAddressTable
OID | Name | Type | Access
.1 | Value | InetAddressIPv6 | R
.2 | DUID | OCTET STRING | R
.3 | LinkPrefixId | INTEGER | R
.4 | IAID | Unsigned32 | R
.5 | PrefLifetime | Unsigned32 | R
.6 | ValidLifetime | Unsigned32 | R
.7 | Age | TimeStamp | R
Value
Assigned address. Length: 16 to 16
DUID
DUID of related DHCPv6-client (see 9 and 22.2 of RFC-3315). An empty dummy-DUID is used for storing addresses from received Decline-messages (see section 5.3 of RFC-33).
LinkPrefixId
'Id' value of related 'ip6LinkPrefix' entry.
IAID
IAID of related IA_NA (see 22.4 of RFC-3315).
PrefLifetime
'Preferred lifetime' in seconds of assigned address (see 22.6 of RFC-3315).
ValidLifetime
'Valid lifetime' in seconds of assigned address (see 22.6 of RFC-3315).
Age
Age of this address-entry.

MIB Reference to Software Version 10.1.21 generated on 2016/12/23. Provided by webmaster@bintec-elmeg.com Copyright ©2016 by bintec elmeg GmbH