>> MIB - Management Information Base
>> Table: sysX8Config - (.1.3.6.1.4.1.272.4.17.3.1)
sysX8Config
OID | Name | Type | Access
.1 | PowerSupply1State | ENUM | R
.2 | PowerSupply1Temp | INTEGER | R
.3 | PowerSupply1TempAlarmThreshold | INTEGER | RW
.4 | PowerSupply1TempAlarmTrap | ENUM | R
.5 | PowerSupply2State | ENUM | R
.6 | PowerSupply2Temp | INTEGER | R
.7 | PowerSupply2TempAlarmThreshold | INTEGER | RW
.8 | PowerSupply2TempAlarmTrap | ENUM | R
.9 | FanControl | ENUM | RW
.10 | FanVersion | DisplayString | R
.11 | Fan1 | INTEGER | R
.12 | Fan2 | INTEGER | R
.13 | Fan3 | INTEGER | R
.14 | Fan4 | INTEGER | R
PowerSupply1State
This variable shows the state of the power supply. Enumerations: missing (1) off (2) running (3) fail (4)
PowerSupply1Temp
This variable shows the actual power supply temperature in the unit Celsius. Range: 0 to 250
PowerSupply1TempAlarmThreshold
Power supply 1 temperature threshold. Range: 0 to 250
PowerSupply1TempAlarmTrap
If the power supply temperature raises above the threshold, a alarm trap is generated every 60 seconds. Enumerations: normal (1) critical (2)
PowerSupply2State
This variable show the the state of the power supply. Enumerations: missing (1) off (2) running (3) fail (4)
PowerSupply2Temp
This variable shows the actual power supply temperature in the unit Celsius. Range: 0 to 250
PowerSupply2TempAlarmThreshold
Power supply 2 temperature threshold. Range: 0 to 250
PowerSupply2TempAlarmTrap
If the power supply temperature raises above the threshold, a alarm trap is generated every 60 seconds. Enumerations: normal (1) critical (2)
FanControl
This variable defines automatic fan control. In mode 'auto' the fans are automatically adjusted depending on the current temperature. In mode 'high' all fans remain at maximum speed. Enumerations: auto (1) high (2)
FanVersion
This variable shows the firmware version of the fan unit. Length: 0 to 255
Fan1
This variable shows the current turning speed.
Fan2
This variable shows the current turning speed.
Fan3
This variable shows the current turning speed.
Fan4
This variable shows the current turning speed.

MIB Reference to Software Version 10.1.21 generated on 2016/12/23. Provided by webmaster@bintec-elmeg.com Copyright ©2016 by bintec elmeg GmbH