>> MIB - Management Information Base
>> Table: snmpAccessRuleTable - (.1.3.6.1.4.1.272.4.22.3.1.10.1)
Description: The snmpAccessRuleTable defines OID specific rules that have to be checked for rule-based users (for users in biboAdmLoginTable with biboAdmLoginSNMPAccessLevel = rule-based).
snmpAccessRuleTable
OID | Name | Type | Access
.1 | Index | INTEGER | RW
.2 | AdminStatus | ENUM | D
.3 | NextRule | INTEGER | RW
.4 | AccessRights | ENUM | RW
.5 | ItemSet | INTEGER | RW
Index
Unique index for this entry. Range: 1 to 65535
AdminStatus
Enable/ disable/ delete this entry. Enumerations: enabled (1) disabled (2) delete (3)
NextRule
This object specifies the index of the next rule in the rule list. If this object is 0, this marks the end of the rule list. Range: 0 to 65535
AccessRights
Defines default SNMP access rights associated with this entry. Available default rights are: no-access(1), read-only(2), read-write(3) These access rights are used when the examined OID matches an OID in ItemSet referred by snmpAccessRuleItemSet of this entry. Default value for this variable is no-access in order to avoid unintentionally granting access rights. Enumerations: no-access (1)
ItemSet
Refers to the index of the first entry in snmpItemSetTable. Range: 1 to 65535

MIB Reference to Software Version 10.1.21 generated on 2016/12/23. Provided by webmaster@bintec-elmeg.com Copyright ©2016 by bintec elmeg GmbH