>> MIB - Management Information Base
>> Table: igmpSrcListTable - (.1.3.6.1.4.1.272.4.5.51.4.1)
Description: An entry (conceptual row) in the igmpSrcListTable.
igmpSrcListTable
OID | Name | Type | Access
.1 | Address | IpAddress | R
.2 | IfIndex | InterfaceIndex | R
.3 | HostAddress | IpAddress | R
.4 | Status | ENUM | D
.5 | Timer | TimeTicks | R
.6 | Self | ENUM | R
Address
The IP multicast group address for which this entry contains information.
IfIndex
The interface for which this entry contains information for an IP multicast group address. Range: 1 to 2147483647
HostAddress
The host address to which this entry corresponds. The CacheSourceFilterMode value for this Group address and interface indicates whether this Host address is included or excluded.
Status
The status of this entry. Enumerations: active (1) notInService (2) notReady (3) createAndGo (4) createAndWait (5) destroy (6)
Timer
The time when this entry will be aged out.
Self
An indication of whether the local system is a member of this entity. Enumerations: true (1) false (2)

MIB Reference to Software Version 10.1.21 generated on 2016/12/23. Provided by webmaster@bintec-elmeg.com Copyright ©2016 by bintec elmeg GmbH