>> MIB - Management Information Base
>> Table: ip6DhcpOptionSetTable - (.1.3.6.1.4.1.272.4.5.100.4.3.1)
Description: Option-sets control what options are 'visible' per incoming message. Each configured option belongs to exactly one option-set (may contain multiple options) which can be assigned to a certain interface or client via its filter-settings. Per incoming message, 'visible options' are selected in two phases. In phase one, 'matching option-sets' are found via filter-settings, and contained options make up list of 'matching options'. In phase two, 'matching options' may 'override' each other, based on option-set-specific prio-settings. If multiple options of same 'type' (i.e. defined in same MIB-table) are matching but have different prios then all entries that do not have highest matching prio are 'overridden' and thus not 'visible'. In a typical scenario, there is one high-prio option-set per interface with some interface-specific options plus one low-prio option-set with some default-options to be visible only if no options of same type are listed for related matching interface. Further option-type-specific requirements (e.g. if related option was listed in 'Option Request Option', see 22.7 of RFC-3315) may have an impact on whether a 'visible option' is also 'processing-relevant'.
ip6DhcpOptionSetTable
OID | Name | Type | Access
.1 | Id | INTEGER | RW
.2 | AdminStatus | ENUM | D
.3 | Description | DisplayString | RW
.4 | Prio | INTEGER | RW
.5 | IfIndex | InterfaceIndexOrZero | RW
.6 | ClientDUID | OCTET STRING | RW
Id
Internal identifier of this option-set. Range: 1 to 65535
AdminStatus
Activate/deactivate/delete this option-set. Enumerations: enabled (1) disabled (2) delete (3)
Description
Textual description of this option-set. Length: 0 to 255
Prio
Priority for the 'override' mechanism described above. Range: 0 to 255
IfIndex
Optional filter-criterion: Rx-interface of processed DHCPv6-frame. A value of 0 means that any Rx-interface matches. Range: 0 to 2147483647
ClientDUID
Optional filter-criterion: Client-DUID of processed DHCPv6-frame (see 9 and 22.2 of RFC-3315). An empty string means that any Client-DUID or even missing DUID matches.

MIB Reference to Software Version 10.1.21 generated on 2016/12/23. Provided by webmaster@bintec-elmeg.com Copyright ©2016 by bintec elmeg GmbH