>> MIB - Management Information Base
>> Table: voipProfileTable - (.1.3.6.1.4.1.272.4.18.3.1)
Description: This Table contains entries for the voice profiles supported by the installed modem.
voipProfileTable
OID | Name | Type | Access
.1 | Name | ENUM | R
.2 | Descr | DisplayString | RW
.3 | Encoding | ENUM | RW
.4 | Encapsulation | ENUM | RW
.5 | EchoCancellation | ENUM | RW
.6 | ComfortNoise | ENUM | RW
.7 | PacketLength | INTEGER | RW
.8 | PacketInterval | INTEGER | RW
.9 | JitterBufferDelay | INTEGER | RW
Name
The name of the profile. A maximum of ten profiles is available depending on the hardware/firmware version and availability of license information. voip-profile-1 (1) : G.711 A-Law + RTP + EchoC voip-profile-2 (2) : G.711 A-Law + RTP + EchoC + CNoise voip-profile-3 (3) : G.711 A-Law + RAW + EchoC voip-profile-4 (4) : G.711 u-Law + RTP + EchoC voip-profile-5 (5) : G.711 u-Law + RTP + EchoC + CNoise voip-profile-6 (6) : G.711 u-Law + RAW + EchoC voip-profile-7 (7) : G.729 A + RTP + EchoC voip-profile-8 (8) : G.729 B + RTP + EchoC(+ CNoise) voip-profile-9 (9) : G.723.1 + RTP + EchoC voip-profile-10 (10) : G.723.1A + RTP + EchoC(+ CNoise) Enumerations: voip-profile-1 (1) voip-profile-2 (2) voip-profile-3 (3) voip-profile-4 (4) voip-profile-5 (5) voip-profile-6 (6) voip-profile-7 (7) voip-profile-8 (8) voip-profile-9 (9) voip-profile-10 (10)
Descr
Profile Description. Info only. Length: 0 to 255
Encoding
This object specifies the preferred voice encoding algorithm. g711uLaw (1) : G.711 u-Law 64.0 kbit/s g711aLaw (2) : G.711 A-Law 64.0 kbit/s g729a (3) : G.729A CS-ACELP 8.0 kbit/s g729b (4) : G.729B ??? g723-63 (5) : G.723.1 MP-MLQ 6.3 kbit/s g723-53 (6) : G.723.1 ACELP 5.3 kbit/s Enumerations: g711uLaw (1) g711aLaw (2) g729a (3) g729b (4) g723-63 (5) g723-53 (6)
Encapsulation
This object specified the encapsulation mode of the voice data. Enumerations: raw (1) rtp (2) aal2 (3)
EchoCancellation
This object enables or disables the G.164 echo cancellation. Enumerations: off (1) on (2)
ComfortNoise
This object enables or disables the voice activity detection and comfort noise generation. none (1) : linear voice stream vad (2) : voice activity detection cng (3) : comfort noise generation vad-cng (4) : vad + cng Enumerations: none (1) vad (2) cng (3) vad-cng (4)
PacketLength
This object defines the default packet length in milliseconds of the different voice compression algorithms. g729 : 10 bytes / 10 ms g723-acelp : 20 bytes / 30 ms g723-mp-mlq : 24 bytes / 30 ms g711 : 80 bytes / 10 ms Range: 10 to 255
PacketInterval
This object specifies the number of ms coded in one voice data packet. Must be a multiple of the time implicitely defined by voipProfilePacketLength above. Range: 10 to 210
JitterBufferDelay
This object specifies the initial delay of the adaptive jitter buffer. Range: 10 to 250

MIB Reference to Software Version 10.1.21 generated on 2016/12/23. Provided by webmaster@bintec-elmeg.com Copyright ©2016 by bintec elmeg GmbH