>> MIB - Management Information Base
>> Table: dspTable - (.1.3.6.1.4.1.272.4.17.4.3.1)
Description: The DspTable contains information about Digital Signal processors in the system.
dspTable
OID | Name | Type | Access
.1 | Slot | INTEGER | R
.2 | Unit | INTEGER | R
.3 | Descr | DisplayString | R
.4 | Capabilities | BITS | R
.5 | TotalChannels | INTEGER | R
.6 | UsedChannels | INTEGER | R
Slot
DSP Slot Number. Range: 0 to 512
Unit
DSP Unit Number. Range: 0 to 9999
Descr
Description of DSP. Length: 0 to 255
Capabilities
This bitfield describes what the DSP supports. Enumerations: g711 (0) g722 (1) g723 (2) g728 (3) g726 (4) g729 (5) ilbc (6) clear (7) t30 (8) t38 (9) dtmf (10)
TotalChannels
Total number of channels of this DSP. Range: 1 to 1000
UsedChannels
Number of used channels of this DSP. Range: 1 to 1000

MIB Reference to Software Version 10.1.21 generated on 2016/12/23. Provided by webmaster@bintec-elmeg.com Copyright ©2016 by bintec elmeg GmbH