>> MIB - Management Information Base
>> Table: usbInterfaceDescTable - (.1.3.6.1.4.1.272.4.55.3.1)
Description: (one entry of usbInterfaceDescTable)
usbInterfaceDescTable
OID | Name | Type | Access
.1 | DevAddr | INTEGER | R
.2 | InterfaceNumber | INTEGER | R
.3 | AltSettings | INTEGER | R
.4 | NumEndpoints | INTEGER | R
.5 | DeviceClass | ENUM | R
.6 | DeviceSubClass | INTEGER | R
.7 | DeviceProtocol | INTEGER | R
.8 | IdxInterface | INTEGER | R
.9 | RawData | OCTET STRING | R
DevAddr
DevAddr = (slot << 12) | (unit << 8) | (Enum << 4). Enum is assigned by the USB device enumerator. Range: 0 to 65535
InterfaceNumber
The number of this interface. Range: 0 to 255
AltSettings
Value used to select alternative setting. Range: 0 to 255
NumEndpoints
The number of endpoints provided by this interface. Range: 0 to 255
DeviceClass
Class code (assigned by usb.org). Enumerations: unspec (0) audio (1) cdc (2) hid (3) physical (5) image (6) printer (7) msc (8) hub (9) cdc-data (10) smartcard (11) firm-upd (12) security (13) diagnostic (220) wireless (224) appl-spec (254) vendor-spec (255)
DeviceSubClass
Subclass code (assigned by usb.org). Range: 0 to 255
DeviceProtocol
The class dependent protocol code. Range: 0 to 255
IdxInterface
The index to the string describing the interface (if present). Range: 0 to 255
RawData
Interface descriptor raw data for debugging purposes only. Length: 0 to 9

MIB Reference to Software Version 10.1.21 generated on 2016/12/23. Provided by webmaster@bintec-elmeg.com Copyright ©2016 by bintec elmeg GmbH