>> MIB - Management Information Base
>> Table: ipDnsServerCfgTable - (.1.3.6.1.4.1.272.4.5.20.32.1)
Description: Contains manually configured nameserver-addresses and automatically added entries for DHCP/IPCP-assigned nameservers.
ipDnsServerCfgTable
OID | Name | Type | Access
.1 | Index | INTEGER | RW
.2 | AdminStatus | ENUM | D
.3 | Mode | ENUM | RW
.4 | Priority | INTEGER | RW
.5 | PrimaryAddress | IpAddress | RW
.6 | SecondaryAddress | IpAddress | RW
.7 | IfIndex | INTEGER | RW
.8 | Description | DisplayString | RW
.9 | Ip6PrimaryAddress | InetAddressIPv6 | RW
.10 | Ip6SecondaryAddress | InetAddressIPv6 | RW
.11 | IpVersion | ENUM | RW
Index
Unique index for unambiguous SNMP-addressing.
AdminStatus
Administrative status of this entry. Enumerations: enabled (1) disabled (2) delete (3)
Mode
Specifies whether nameserver-addresses are configured manually or updated automatically (see ipDnsDynamicGlobals) with each IPCP/DHCP-negotiation. Enumerations: manual (1) automatic (2)
Priority
Relative priority (0 is highest) of this entry. Range: 0 to 9
PrimaryAddress
IP-address of primary nameserver. Relevant only for manual entries (0 for automatic ones).
SecondaryAddress
IP-address of secondary nameserver. Relevant only for manual entries (0 for automatic ones).
IfIndex
Index of interface where nameservers are DHCP/IPCP-assigned. Relevant only for automatic entries (-1 for manual ones).
Description
Optional textual description for this nameserver-entry. Length: 0 to 64
Ip6PrimaryAddress
The primary DNS Server IPv6 Address.
Ip6SecondaryAddress
The secondary DNS Server IPv6 Address.
IpVersion
Determines whether the IPv4 or IPv6 DNS Server address pair should be considered. In dynamic case (DHCP/IPCP-assigned) either IPv4 or IPv6 DNS addresses will be filled into the associated ipDnsServerOperEntry.

MIB Reference to Software Version 10.1.21 generated on 2016/12/23. Provided by webmaster@bintec-elmeg.com Copyright ©2016 by bintec elmeg GmbH