>> MIB - Management Information Base
>> Table: ip6AdmAddrTable - (.1.3.6.1.4.1.272.4.5.100.1.3.1)
Description: A static address entry.
ip6AdmAddrTable
OID | Name | Type | Access
.1 | Address | InetAddressIPv6 | RW
.2 | Length | INTEGER | RW
.3 | IfIndex | InterfaceIndex | RW
.4 | AdminStatus | ENUM | D
.5 | LkPrefixId | INTEGER | RW
Address
The destination IPv6 address of this route. This object may not take a multicast address value. Length: 16 to 16
Length
Indicates the prefix length of the address. Range: 1 to 128
IfIndex
Indicates the Interface the address belongs to. Range: 1 to 2147483647
AdminStatus
The Administration state of the address entry. Enumerations: enable (1) disable (2) delete (3)
LkPrefixId
Referenece to ipLinkPrefixTable entries, used in order to merge the static (host) part of this address with the associated (probably dynamic) link prefix.

MIB Reference to Software Version 10.1.21 generated on 2016/12/23. Provided by webmaster@bintec-elmeg.com Copyright ©2016 by bintec elmeg GmbH