>> MIB - Management Information Base
>> Table: voip - (.1.3.6.1.4.1.272.4.33)
voip
OID | Name | Type | Access
.6 | voipSip | sip | N
.10 | CallHistoryMaxEntries | INTEGER | RW
.11 | AdminStatus | ENUM | RW
.22 | voipStatMIB | voip | N
.1 | DialLatency | INTEGER | RW
.2 | Termination | ENUM | RW
.3 | OperStatus | ENUM | R
.4 | LastError | DisplayString | R
.5 | SBC | INTEGER | RW
.6 | DropExtension | DisplayString | RW
.1 | voipStatRtcpHistoryMaxEntries | INTEGER | RW
.20 | ServerCertIndex | INTEGER | RW
.21 | ServerCertSource | ENUM | RW
.22 | MaxConcurrentServerTransactions | INTEGER | RW
.23 | MaxServerTransactionsPerSecond | INTEGER | RW
.24 | MaxServerTransactionsPerPeer | INTEGER | RW
.25 | RoutingPreference | ENUM | RW
.26 | DefaultCountryCode | DisplayString | RW
.27 | DefaultAreaCode | DisplayString | RW
.28 | SipPort | INTEGER | RW
.29 | SipNatPort | INTEGER | RW
.30 | DscpSignalling | INTEGER | RW
.31 | IsdnTypeOfNumber | ENUM | RW
voipSip
description not available
CallHistoryMaxEntries
Maximum number of voipCallHistory entries in memory. Range: 0 to 65535
AdminStatus
Globally enable or disable VoIP features. Setting this to 'disable' disables all VoIP dependent subsystems including Mediagateway. Enumerations: disabled (1) enabled (2)
voipStatMIB
description not available
DialLatency
The dial delay in seconds after the last entered digit. Range: 1 to 15
Termination
This value describes the RTP stream routing between SIP phones: 'off' -> RTP streams between phones are routed directly; 'on' -> RTP streams are always terminated in the gateway. This value can be set to off to reduce systemload. In this case all SIP phones in the network must be able to connect over IP routing. Otherwise the Mediagateway is always endpoint of the RTP stream and the streams are connected in the gateway. Enumerations: off (1) on (2)
OperStatus
The operational status of the Mediagateway. Enumerations: down (1) up (2) failed (3)
LastError
The last error message on PABX startup. Length: 0 to 255
SBC
Set the default Session Border Controller (SBC) behaviour. A Session Border Controller is a SIP provider account which takes over the PBX functionality of the Mediagateway. The 'DDIMode' of the used SIP provider account has to be anything but 'off'. All internal and external activities are controlled by the SBC. If the SBC is disabled ('-1') or the SBC is not available the Mediagateway uses the internal PBX functionality. Auto mode ('0') means that a separate SIP account is used for each existing extension entry (so in this case it is not possible to set one global SBC). In auto mode each voipExtensionTable entry needs a matching voipProviderTable/voipSipProviderTable entry. So in auto mode Mediagateway pairs SIP provider accounts and their matching extensions. Possible values: -1 -> SBC is disabled; 0 -> Auto mode; 1...999 -> Index of a voipSipProviderTable entry (has to be a SIP trunk provider).
DropExtension
Fallback number which is dialed if no matching call endpoint (extension) for a dialed number is found. Fallback number can be an internal extension or another external call endpoint. Length: 0 to 255
voipStatRtcpHistoryMaxEntries
Maximum number of voipStatRtcpHistory entries in memory. Range: 0 to 65535
ServerCertIndex
Index of certificate entry in certTable which is to be used as server certificate for SIPS transport. This parameter is only used if 'ServerCertSource' = 'certtable'.
ServerCertSource
Source of server certificate for SIPS transport: 'internal' -> 'ServerCertIndex' is not used, internal server certificate of SIP stack is used instead; 'certtable' -> use certificate from certTable entry specified by 'ServerCertIndex'. Default value is 'internal'. Enumerations: internal (1) certtable (2)
MaxConcurrentServerTransactions
The maximum amount of concurrent server transactions created by incoming INVITE, REGISTER, ... If the limit is reached, new server transactions will be ignored. A value of 0 means no limitation Range: 0 to 10000
MaxServerTransactionsPerSecond
The maximum amount of server transactions per second created by incoming INVITE, REGISTER, ... If the limit is reached, new server transactions will be ignored. A value of 0 means no limitation Range: 0 to 10000
MaxServerTransactionsPerPeer
The maximum amount of server transactions per peer created by incoming INVITE, REGISTER, ... If the limit is reached, new server transactions from that peer will be ignored. A value of 0 means no limitation Range: 0 to 10000
RoutingPreference
The routing preference for the received called address. - local matching local extensions are preferred - routing matching configured routes are preferred Enumerations: local (1) routing (2)
DefaultCountryCode
The default country code. This value is used by GUI VoIP configuration to set or modify provider specific dialing rules. Length: 0 to 6
DefaultAreaCode
The default area code. This value is used by GUI VoIP configuration to set or modify provider specific dialing rules. Length: 0 to 12
SipPort
Standard value of the SIP port. Range: 0 to 65535
SipNatPort
The external port mapped by NAT. For security reasons this might be different than the internal port (mpsVoIPConfigSipPort). Range: 0 to 65535
DscpSignalling
The 6 bit DSCP value used in IP header for signalling data. Range: 0 to 63
IsdnTypeOfNumber
Specifies the type of of number for the calling number in ISDN setup: standard - calling number is not modified and type of number is unknown. specific - calling number is checked for international, national or subscriber. The type of number is set to the result. The calling number is modified if the type is international or national. Enumerations: standard (1) specific (2)

MIB Reference to Software Version 10.1.21 generated on 2016/12/23. Provided by webmaster@bintec-elmeg.com Copyright ©2016 by bintec elmeg GmbH