>> MIB - Management Information Base
>> Table: ip6RouteTable - (.1.3.6.1.4.1.272.4.5.100.2.5.1)
Description: A routing entry.
ip6RouteTable
OID | Name | Type | Access
.1 | Target | InetAddressIPv6 | R
.2 | TargetLen | INTEGER | R
.3 | Source | InetAddressIPv6 | R
.4 | SourceLen | INTEGER | R
.5 | IfIndex | InterfaceIndexOrZero | R
.6 | NextHop | InetAddressIPv6 | R
.7 | Protocol | ENUM | R
.8 | Metric | Unsigned32 | R
.9 | Lifetime | Unsigned32 | R
.10 | Prefix | Integer32 | R
.11 | Age | TimeStamp | R
Target
The destination IPv6 address of this route. This object may not take a multicast address value. Length: 16 to 16
TargetLen
Indicates the prefix length of the destination address. Range: 0 to 128
Source
The Source IPv6 address of this route. This object may not take a multicast address value. Length: 16 to 16
SourceLen
Indicates the prefix length of the source address. Range: 0 to 128
IfIndex
The index value which uniquely identifies the local interface through which the next hop of this route should be reached. The interface identified by a particular value of this index is the same interface as identified by the same value of ip6AdmIfIfIndex. For routes of the discard type this value can be zero. Range: 0 to 2147483647
NextHop
On remote routes, the address of the next hop of this routing entry, set to :: otherwise. Length: 16 to 16
Protocol
The routing mechanism via which this route was learned. Enumerations: static (1) netmgmt (2) ndisc (3) rip (4) ospf (5) bgp (6) idrp (7) dhcp-pd (8)
Metric
The routing metric for this route. The semantics of this metric are determined by the routing protocol specified in the route's ip6RouteProtocol value. When this is unknown or not relevant to the protocol indicated by ip6RouteProtocol, the object value should be set to its maximum value (4,294,967,295).
Lifetime
The number of seconds the routing entry is valid,
Prefix
The value which identifies the global prefix of the source address using this route.
Age
The number of seconds since this route was last updated or otherwise determined to be correct. Note that no semantics of `too old' can be implied except through knowledge of the routing protocol by which the route was learned.

MIB Reference to Software Version 10.1.21 generated on 2016/12/23. Provided by webmaster@bintec-elmeg.com Copyright ©2016 by bintec elmeg GmbH