>> MIB - Management Information Base
>> Table: bacPropertyTable - (.1.3.6.1.4.1.272.4.60.1.1.1)
Description: One entry in bacPropertyTable
bacPropertyTable
OID | Name | Type | Access
.1 | Index | INTEGER | RW
.2 | Descr | DisplayString | RW
.3 | ParentIndex | INTEGER | RW
.4 | DscpSignalling | INTEGER | RW
.5 | DscpAudio | INTEGER | RW
.6 | BwConfigUp | INTEGER | RW
.7 | BwConfigDown | INTEGER | RW
.8 | AdminStatus | ENUM | D
Index
The index in this property table. Range: 1 to 65535
Descr
The description of the bandwidth property entry. Length: 0 to 255
ParentIndex
The index of the parent BAC property. Is 0, if no parent defined. Range: 0 to 65535
DscpSignalling
The 6 bit DSCP value used in IP header for signalling data. Range: 0 to 63
DscpAudio
The 6 bit DSCP value used IP header for media data. Range: 0 to 63
BwConfigUp
The configured bandwidth for up direction.
BwConfigDown
The configured bandwidth for down direction.
AdminStatus
If the AdminStatus is set to enabled(1) this entry will be used, if set to disabled(2) it won't be used. You may also delete this entry by changing it to delete(3). Enumerations: enabled (1) disabled (2) delete (3)

MIB Reference to Software Version 10.1.21 generated on 2016/12/23. Provided by webmaster@bintec-elmeg.com Copyright ©2016 by bintec elmeg GmbH