>> MIB - Management Information Base
>> Table: userAlert - (.1.3.6.1.4.1.272.4.62.1.2)
userAlert
OID | Name | Type | Access
.1 | AdminStatus | ENUM | RW
.2 | SMTPHost | DisplayString | RW
.3 | Origin | DisplayString | RW
.4 | Mails | INTEGER | RW
.5 | Error | DisplayString | R
.6 | Authentication | ENUM | RW
.7 | POP3Host | DisplayString | RW
.8 | POP3valid | INTEGER | RW
.9 | User | DisplayString | RW
.10 | Pass | DisplayString | RW
.11 | SMSDevice | DisplayString | RW
.12 | SmsPerDay | INTEGER | RW
.13 | SSL | ENUM | RW
.14 | ServerPort | INTEGER | RW
AdminStatus
Disable or enable user Alert service.
SMTPHost
SMTP Server for outgoing emails.
Origin
The name which is used as originator of the email.
Mails
The maximum number of mails sent within one minute.
Error
Displays last SMTP error.
Authentication
SMTP server authentication mode.
POP3Host
POP3 server for SMTP after POP.
POP3valid
The time slot in which mail could be sent via SMTP after POP3 login.
User
Username for SMTP login.
Pass
Password for SMTP login.
SMSDevice
The ICC-ID of the SIM-Card used to sent SMS if present.
SmsPerDay
The maximum number of SMS sent within one day (24 hours). The special value `0' allows unlimited SMS distribution.
SSL
Disable or enable SSL.
ServerPort
SMTP Server port for outgoing emails.

MIB Reference to Software Version 10.1.21 generated on 2016/12/23. Provided by webmaster@bintec-elmeg.com Copyright ©2016 by bintec elmeg GmbH